{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","49","","","52"]
["","","","Bas","dBA","46","","","49"]
["","Rafraîchissement","","Bas","dBA","46","","","49"]
["","","","Haut","dBA","49","","","52"]
["Accessoires standard","manchon d’évacuation","","","","1","","","1"]
["","Manuel d'installation","","","","1","","","1"]
["Réfrigérant","Charge","","","TCO2Eq","3.1","","","4.8"]
["","PRP","","","","2,087.5","","","2,087.5"]
["","Charge","","","kg","1.5","","","2.3"]
["","Type","","","","R-410A","","","R-410A"]
["Raccordements de tuyauterie","Dénivelé","UI - UE","Max.","m","20","","","20"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 10 m)","","","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["Compresseur","Type","","","","Compresseur swing hermétique","","","Compresseur swing hermétique"]
["Dimensions","Unité","","Largeur","mm","825","","","900"]
["","","","Profondeur","mm","300","","","320"]
["","","","Hauteur","mm","735","","","770"]
["Poids","Unité","","","kg","48","","","71"]
["Power supply","Phase","","","","1~","","","1~"]
["","Fréquence","","","Hz","50","","","50"]
["","Tension","","","V","220-240","","","220-240"]
["Remarques","","","","","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)","(1) - 220V","","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)","(1) - 220V"]
["","","","","","(2) - Contient des gaz à effet de serre fluorés.","(2) - 230 V","","(2) - Contient des gaz à effet de serre fluorés.","(2) - 230 V"]
["Dimensions","Unité","","Hauteur","mm","","735","735","","770","770"]
["","","","Largeur","mm","","825","825","","900","900"]
["","","","Profondeur","mm","","300","300","","320","320"]
["Poids","Unité","","","kg","","48","48","","71","71"]
["Compresseur","Type","","","","","Compresseur swing hermétique","Compresseur swing hermétique","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ambiante","Min.","°CBS","","-10","-10","","-10","-10"]
["","","","Max.","°CBS","","46","46","","46","46"]
["","Chauffage","Temp. ambiante","Min.","°CBH","","-15","-15","","-15","-15"]
["","","","Max.","°CBH","","18","20","","18","20"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","49","49","","52","52"]
["","","","Bas","dBA","","46","46","","49","49"]
["","Chauffage","","Haut","dBA","","49","49","","52","52"]
["","","","Bas","dBA","","46","46","","49","49"]
["Réfrigérant","Type","","","","","R-410A","R-410A","","R-410A","R-410A"]
["","Charge","","","kg","","1.5","1.5","","2.3","2.3"]
["","Charge","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["","PRP","","","","","2087.5","2087.5","","2087.5","2087.5"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","","30","30","","30","30"]
["","Charge de réfrigérant supplémentaire","","","kg/m","","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["","Dénivelé","UI - UE","Max.","m","","20","20","","20","20"]
["Accessoires standard","Installation manual","","","","","Installation manual","1","","Installation manual","1"]
["","Drain plug","","","","","Drain plug","","","Drain plug"]
["Alimentation électrique","Phase","","","","","1~","1~","","1~","1~"]
["","Fréquence","","","Hz","","50","50","","50","50"]
["","Tension","","","V","","220-240","220-240","","220-240","220-240"]
["Remarques","","","","","","(3) - 240V","","","(3) - 240V"]
["Accessoires standard","Drain socket","","","","","","1","","","1"]
["Sound power level","Rafraîchissement","","","dBA","","","","65"]