{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F8"]
[]
[]
[]
[]
["","","","","","RXS71FAV1B8"]
["Ventilateur","Débit d’air","Rafraîchissement","Extra lent","m³/min","46.0"]
["","","Chauffage","Extra lent","m³/min","46.0"]
["","","","Extra lent","cfm","1624"]
["","","Chauffage","Extra lent","cfm","1624"]
["Dimensions","Unité","","Hauteur","mm","770"]
["","","","Largeur","mm","900"]
["","","","Profondeur","mm","320"]
["Poids","Unité","","","kg","71"]
["Moteur de ventilateur","Vitesse","Rafraîchissement","Extra lent","tr/min","730"]
["","","Chauffage","Extra lent","tr/min","730"]
["Compresseur","Type","","","","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ambiante","Min.","°CBS","-10"]
["","","","Max.","°CBS","46"]
["","Chauffage","Temp. ambiante","Min.","°CWB","-15"]
["","","","Max.","°CWB","18"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","52"]
["","Chauffage","","Haut","dBA","52"]
["Réfrigérant","Type","","","","R-410A"]
["","Charge","","","kg","2.3"]
["","Charge","","","tCO2Eq","4.8"]
["","PRP","","","","2087.5"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","30"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["","Dénivelé","UI - UE","Max.","m","20"]
["Accessoires standard","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain socket assy","","","","1"]
["Alimentation électrique","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Tension","","","V","220-240"]
["Remarques","","","","","(1) - 220V"]
["","","","","","(2) - 230 V"]
["","","","","","(3) - 240V"]