{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-A"]
[]
[]
[]
[]
["","","","","","RZAG35A2V1B","RZAG50A2V1B","RZAG60A2V1B"]
["Dimensions","Unité","","Hauteur","mm","734","734","734"]
["","","","Largeur","mm","870","870","870"]
["","","","Profondeur","mm","373","373","373"]
["Poids","Unité","","","kg","52","52","52"]
["Compresseur","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","62.0","63.0","64.0"]
["","Chauffage","","","dBA","62.0","63.0","64.0"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","48.0","49.0","50.0"]
["","Chauffage","","Nom.","dBA","48.0","49.0","50.0"]
["Réfrigérant","Type","","","","R-32","R-32","R-32"]
["","Charge","","","kg","1.55","1.55","1.55"]
["","PRP","","","","675.0","675.0","675.0"]
["","Charge","","","tCO2Eq","1.05","1.05","1.05"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35","6.35"]
["","Gaz","","DE","mm","9.50","12.7","12.7"]
["","Longueur de tuyauterie","Max.","UE - UI","m","50","50","50"]
["","","Système","Sans charge","m","30","30","30"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 30 m)","0,02 (pour longueur de tuyauterie supérieure à 30 m)","0,02 (pour longueur de tuyauterie supérieure à 30 m)"]
["","Dénivelé","UI - UE","Max.","m","30.0","30.0","30.0"]
["Accessoires standard","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Alimentation électrique","Phase","","","","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50"]
["","Tension","","","V","220-240","220-240","220-240"]