{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-B"]
[]
[]
[]
[]
["","","","","","RZAG35B5V1B","RZAG50B5V1B","RZAG60B5V1B"]
["Dimensions","Unité","","Hauteur","mm","734","734","734"]
["","","","Largeur","mm","870","870","870"]
["","","","Profondeur","mm","373","373","373"]
["Poids","Unité","","","kg","52","52","52"]
["Compresseur","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ambiante","Min.","°CBS","-20","-20","-20"]
["","","","Max.","°CBS","52","52","52"]
["","Chauffage","Temp. ambiante","Min.","°CBH","-21","-21","-21"]
["","","","Max.","°CBH","18","18","18"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","62","63","64"]
["","Chauffage","","","dBA","62","63","64"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","48","49","50"]
["","Chauffage","","Nom.","dBA","48","49","50"]
["Réfrigérant","Type","","","","R-32","R-32","R-32"]
["","Charge","","","kg","1.55","1.55","1.55"]
["","PRP","","","","675","675","675"]
["","Charge","","","tCO2Eq","1.05","1.05","1.05"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35","6.35"]
["","Gaz","","DE","mm","9.52","12.7","12.7"]
["","Longueur de tuyauterie","Max.","UE - UI","m","50","50","50"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 30 m)","0,02 (pour longueur de tuyauterie supérieure à 30 m)","0,02 (pour longueur de tuyauterie supérieure à 30 m)"]
["","Dénivelé","UI - UE","Max.","m","30","30","30"]
["Accessoires standard","RZAG35B5V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","General safety precautions","General safety precautions","General safety precautions"]
["","LOT10 Energy Label","","","","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Alimentation électrique","Phase","","","","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50"]
["","Tension","","","V","220-240","220-240","220-240"]
["Remarques","","","","","(1) - Voir le schéma séparé pour la plage de fonctionnement","(1) - Voir le schéma séparé pour la plage de fonctionnement","(1) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","","(2) - Pour les données électriques, se reporter au schéma séparé.","(2) - Pour les données électriques, se reporter au schéma séparé.","(2) - Pour les données électriques, se reporter au schéma séparé."]
["","","","","","(3) - Contient des gaz à effet de serre fluorés.","(3) - Contient des gaz à effet de serre fluorés.","(3) - Contient des gaz à effet de serre fluorés."]
["Accessoires standard","RZAG50B5V1B","","","","","1"]
["","RZAG60B5V1B","","","","","","1"]