{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":57,"n_cols":7,"rows_kept":57,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Dimensions","Unité","","Hauteur","mm","1,680"]
["","","","Largeur","mm","930"]
["","","","Profondeur","mm","765"]
["Poids","Unité","","","kg","183.0"]
["Compresseur","Type","","","","Compresseur scroll hermétique"]
["Plage de fonctionnement","Rafraîch.","Temp. ambiante","Min.","°CBS","-5.0"]
["","","","Max.","°CBS","46.0"]
["","Heating","Temp. ambiante","Min.","°CBH","-15.0"]
["","","","Max.","°CBH","15.0"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","78.0"]
["","Chauffage","","","dBA","78.0"]
["Réfrigérant","Type","","","","R-410A"]
["","Charge","","","kg","8.3"]
["","PRP","","","","2,087.5"]
["Raccords de tuyauterie","Liquide","","DE","mm","9.52"]
["","Gaz","","DE","mm","22.2"]
["","Longueur de tuyauterie","Max.","UE - UI","m","100"]
["","","Système","Sans charge","m","30"]
["Accessoires standard","Manuel d'installation","","","","1"]
["","Tuyaux de raccordement","","","","4"]
["Power supply","Phase","","","","3N~"]
["","Fréquence","","","Hz","50"]
["","Tension","","","V","380-415"]
["Courant - 50 Hz","Intensité maximale de fusible (MFA)","","","A","25"]
["Remarques","","","","","(1) - L'alimentation électrique de l'unité intérieure FDQ est distincte."]
["","","","","","(2) - Pour les données électriques, se reporter aux schémas séparés."]
["Dimensions","Unité","","Hauteur","mm","","1680"]
["","","","Largeur","mm","","930"]
["","","","Profondeur","mm","","765"]
["Poids","Unité","","","kg","","184.0"]
["Compresseur","Type","","","","","Compresseur scroll hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ambiante","Min.","°CBS","","-5.0"]
["","","","Max.","°CBS","","46.0"]
["","Chauffage","Temp. ambiante","Min.","°CBH","","-15.0"]
["","","","Max.","°CBH","","15.0"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","","78.0"]
["","Chauffage","","","dBA","","78.0"]
["Réfrigérant","Type","","","","","R-410A"]
["","Charge","","","kg","","9.3"]
["","PRP","","","","","2087.5"]
["","Charge","","","tCO2Eq","","19.4"]
["Raccords de tuyauterie","Liquide","","DE","mm","","12.70"]
["","Gaz","","DE","mm","","22.2"]
["","Longueur de tuyauterie","Max.","UE - UI","m","","100"]
["","","Système","Sans charge","m","","30"]
["Accessoires standard","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Alimentation électrique","Phase","","","","","3N~"]
["","Fréquence","","","Hz","","50"]
["","Tension","","","V","","380-415"]
["Courant&nbsp;- 50&nbsp;Hz","Courant&nbsp;- 50&nbsp;Hz-=-Intensité maximale de fusible (MFA)-=-A","","","A","","25"]