{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M"]
[]
[]
[]
[]
["","","","","","2AMXM40M3V1B","2AMXM40M4V1B","2AMXM40M2V1B","2AMXM50M2V1B","2AMXM50M4V1B","2AMXM50M3V1B"]
["Ventilator","Luchtdebiet","Koelen","Superlaag","m³/min","","","30","34"]
["","","Verwarmen","Superlaag","m³/min","","","32","34"]
["Geluidsvermogenniveau","Verwarmen","","","dBA","","62","","","62"]
["","Koelen","","","dBA","","60","","","60"]
["Ventilator","Luchtdebiet","Koelen","Superlaag","cfm","","","1059","1200"]
["","","Verwarmen","Superlaag","cfm","","","1130","1200"]
["Afmetingen","Unit","","Hoogte","mm","550","550","550","550","550","550"]
["","","","Breedte","mm","765","765","765","765","765","765"]
["","","","Diepte","mm","285","285","285","285","285","285"]
["Gewicht","Unit","","","kg","36","36","36","41","41","41"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm","500","500","760","890","500","500"]
["","","Verwarmen","Superlaag","tpm","320","320","820","890","500","500"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°C DB","","46.0","-10","-10","46.0"]
["","","","Max.","°C DB","","-10","46","46","-10"]
["","Verwarmen","Omgeving","Min.","°CWB","","-15","-15","-15","-15.0"]
["","","","Max.","°CWB","","18.0","18","18","18.0"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","46","46","","","48","48"]
["","","","Nom.","dBA","","","48","46"]
["","Verwarmen","","Hoog","dBA","48","48","","","50","50"]
["","","","Nom.","dBA","","","50","48"]
["Koelmiddel","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Vulling","","","kg","0.88","0.88","0.88","1.15","1.15","1.15"]
["Koudemiddel","Vulling","","","tCO2Eq","0.59","0.6","0.6","0.8","0.78","0.78"]
["Koelmiddel","GWP","","","","675.0","675","675","675","675","675"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","20","20 (1)","20","20","20 (1)","20"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 20 m)","0,02 (voor leidinglengte van meer dan 20 m)","002 (voor leidinglengte van meer dan 20 m)","0,02 (voor leidinglengte van meer dan 20 m)","0,02 (voor leidinglengte van meer dan 20 m)","0,02 (voor leidinglengte van meer dan 20 m)"]
["","Niveauverschil:","IU - OU","Max.","m","15.0","15","15","15","15","15.0"]
["","","IU - IU","Max.","m","7.5","7.5","7.5","7.5","7.5","7.5"]
["","Totale leidinglengte","Systeem","Werkelijk","m","30","30","30","30","30","30"]
["Standaard-accessoires","Installation manual","","","","1","1","Installation manual","1","1","1"]
["","Drain plug","","","","1","1","Drain plug","1","1","1"]
["","Screw bag","","","","1","1","Screw bag","1","1","1"]
["Voeding","Fase","","","","1~","1~","1~","1~","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50","50","50","50","50"]
["","Spanning","","","V","220-230-240","220-230-240","220-240","220-240","220-230-240","220-230-240"]
["Opmerkingen","","","","","(1) - Van één kamer","","(1) - Bevat gefluoreerde broeikasgassen","","","(1) - Van één kamer"]
["","","","","","","(1) - Van één kamer","","","(1) - Van één kamer"]
["","","","","","","(2) - Zie afzonderlijke afbeelding voor bedrijfsbereik","","","(2) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","","(3) - Voor elektrische gegevens zie afzonderlijke tekening","","","(3) - Voor elektrische gegevens zie afzonderlijke tekening"]
["","","","","","","(4) - Bevat gefluoreerde broeikasgassen","","","(4) - Bevat gefluoreerde broeikasgassen"]
["Standaard-accessoires","Reducer assembly","","","","","","","1","1","1"]