{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-M"]
[]
[]
[]
[]
["","","","","","3MXM40M2V1B","3MXM52M2V1B","3MXM68M2V1B"]
["Ventilator","Luchtdebiet","Koelen","Superlaag","m³/min","24","24","24.1"]
["","","Verwarmen","Superlaag","m³/min","24","24","24.1"]
["","","","Superlaag","cfm","847","847","851"]
["","","Verwarmen","Superlaag","cfm","847","847","851"]
["Afmetingen","Unit","","Hoogte","mm","734","734","734"]
["","","","Breedte","mm","868","868","868"]
["","","","Diepte","mm","320","320","320"]
["Gewicht","Unit","","","kg","57","57","62"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm_","420","420"]
["","","Verwarmen","Superlaag","tpm_","420","420"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°CDB","-10","-10","-10"]
["","","","Max.","°CDB","46","46","46"]
["","Verwarmen","Omgeving","Min.","°CWB","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18"]
["Geluidsdrukniveau","Koelen","","Nom.","dBA","46","46","48"]
["","Verwarmen","","Nom.","dBA","47","47","48"]
["Koelmiddel","Type","","","","R-32","R-32","R-32"]
["","Vulling","","","kg","1.80","1.80","2.0"]
["Koudemiddel","Vulling","","","tCO2Eq","1.2","1.2","1.4"]
["Koelmiddel","GWP","","","","675","675","675"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","25","25","25"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 30 m)","0,02 (voor leidinglengte van meer dan 30 m)"]
["","Niveauverschil:","IU - OU","Max.","m","15","15","15"]
["","","IU - IU","Max.","m","7.5","7.5","7.5"]
["","Totale leidinglengte","Systeem","Werkelijk","m","50","50"]
["Standaard-accessoires","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Voeding","Fase","","","","1~","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240"]
["Standaard-accessoires","Drain cap","","","","","","9"]
["","Reducer assembly","","","","","","1"]