{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":8,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXS-G"]
[]
[]
[]
[]
["","","","","","3MXS68G3V1B2","3MXS68G3V1B","3MXS68G2V1B"]
["Geluidsdrukniveau","Verwarmen","","Nom.","dBA","49","49"]
["","Koelen","","Nom.","dBA","48","48"]
["Standaard-accessoires","Montagehandleiding","","","","1","1"]
["","Aftapplug","","","","1","1"]
["","Montage verloopstuk","","","","1","1"]
["","Regelplaat voor luchtstroomrichting","","","","Regelplaat voor luchtstroomrichting","Regelplaat voor luchtstroomrichting"]
["Koelmiddel","Charge","","","TCO2Eq","5.4","5.4"]
["","GWP","","","","2,087.5","2,087.5"]
["","Charge","","","kg","2.59","2.59"]
["","Type","","","","R-410A","R-410A"]
["Leidingaansluitingen","Niveauverschil:","IU - IU","Max.","m","7.5","7.5"]
["","","IU - OU","Max.","m","15","15"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 30 m)","0,02 (voor leidinglengte van meer dan 30 m)"]
["","Totale leidinglengte","Systeem","Werkelijk","m","50","50"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Afmetingen","Unit","","Breedte","mm","936","936"]
["","","","Diepte","mm","300","300"]
["","","","Hoogte","mm","735","735"]
["Gewicht","Unit","","","kg","58","58"]
["Power supply","Phase","","","","1~","1~"]
["","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","230","230"]
["Opmerkingen","","","","","(1) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB; equivalente leidinglengte: 5m","(1) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB; equivalente leidinglengte: 5m"]
["","","","","","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m"]
["","","","","","(3) - Bevat gefluoreerde broeikasgassen","(3) - Bevat gefluoreerde broeikasgassen"]
["Afmetingen","Unit","","Hoogte","mm","","","735"]
["","","","Breedte","mm","","","936"]
["","","","Diepte","mm","","","300"]
["Gewicht","Unit","","","kg","","","58"]
["Compressor","Type","","","","","","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°CDB","","","-10"]
["","","","Max.","°CDB","","","46"]
["","Verwarmen","Omgeving","Min.","°CWB","","","-15"]
["","","","Max.","°CWB","","","15.5"]
["Geluidsdrukniveau","Koelen","","Nom.","dBA","","","48"]
["","Verwarmen","","Nom.","dBA","","","49"]
["Koelmiddel","Type","","","","","","R-410A"]
["","Vulling","","","kg","","","2.59"]
["Koudemiddel","Vulling","","","tCO2Eq","","","5.4"]
["Koelmiddel","GWP","","","","","","2087.5"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","","","25"]
["","Bijkomende koelmiddelvulling","","","kg/m","","","0,02 (voor leidinglengte van meer dan 30 m)"]
["","Niveauverschil:","IU - OU","Max.","m","","","15"]
["","","IU - IU","Max.","m","","","7.5"]
["","Totale leidinglengte","Systeem","Werkelijk","m","","","50"]
["Standaard-accessoires","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["","Air direction adjustment plate","","","","","","Air direction adjustment plate"]
["Voeding","Fase","","","","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","","","50"]
["","Spanning","","","V","","","230"]