{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MWXM-A9"]
[]
[]
[]
[]
["","","","","","5MWXM68A2V1B9","5MWXM90A2V1B9"]
["Afmetingen","Unit","","Hoogte","mm","734","734"]
["","","","Breedte","mm","1,040","1,040"]
["","","","Diepte","mm","408","408"]
["Gewicht","Unit","","","kg","69","73"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["Geluidsdrukniveau","Koelen","","Nom.","dBA","48","52"]
["","Verwarmen","","Nom.","dBA","49","53"]
["Koelmiddel","Type","","","","R-32","R-32"]
["","Vulling","","","kg","2","2.4"]
["Koudemiddel","Vulling","","","tCO2Eq","1.35","1.62"]
["Koelmiddel","GWP","","","","675","675"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","25 (2)","25 (3)"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 30 m)","0,02 (voor leidinglengte van meer dan 30 m)"]
["","Niveauverschil:","IU - OU","Max.","m","15 (3)","15"]
["","","IU - IU","Max.","m","7.5 (3)","7.5 (3)"]
["","Totale leidinglengte","Systeem","Werkelijk","m","60","75"]
["Standaard-accessoires","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","2","2"]
["Voeding","Fase","","","","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","220-440","220-240"]
["Opmerkingen","","","","","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","(2) - Van één kamer","(2) - Van één kamer"]
["","","","","","(3) - Voor één ruimte (raadpleeg de installatiehandleiding voor combinatie met FBA71/100/125 en EKHWET en CKHWS)","(3) - Voor één ruimte (raadpleeg de installatiehandleiding voor combinatie met FBA71/100/125 en EKHWET en CKHWS)"]
["","","","","","(4) - Bevat gefluoreerde broeikasgassen","(4) - Bevat gefluoreerde broeikasgassen"]