{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":8,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXS-E"]
[]
[]
[]
[]
["","","","","","5MXS90E3V3B2","5MXS90E3V3B","5MXS90E7V3B"]
["Geluidsdrukniveau","Verwarmen","","Nom.","dBA","52","52"]
["","Koelen","","Nom.","dBA","52","52"]
["Standaard-accessoires","Montagehandleiding","","","","1","1"]
["","Aftapplug","","","","1","1"]
["","Montage verloopstuk","","","","1","1"]
["Koelmiddel","Charge","","","TCO2Eq","6.2","6.2"]
["","GWP","","","","2,087.5","2,087.5"]
["","Vulling","","","kg","2.99","2.99"]
["","Type","","","","R-410A","R-410A"]
["Werkbereik","Koelen","Omgeving","Max.","°CDB","46"]
["","","","Min.","°CDB","-10"]
["","Heating","Omgeving","Max.","°CWB","18"]
["","","","Min.","°CWB","-15"]
["Leidingaansluitingen","Niveauverschil:","IU - IU","Max.","m","7.5"]
["","","IU - OU","Max.","m","15"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 30 m)"]
["","Totale leidinglengte","Systeem","Werkelijk","m","75"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor"]
["Afmetingen","Unit","","Breedte","mm","900","900"]
["","","","Diepte","mm","320","320"]
["","","","Hoogte","mm","770","770"]
["Gewicht","Unit","","","kg","73","73"]
["Power supply","Phase","","","","1~","1~"]
["","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","230","230"]
["Opmerkingen","","","","","(1) - Koelen: binnentemp. 27 °CDB, 19,0 °CNB, buitentemp. 35 °CDB; equivalente leidinglengte: 7,5m","(1) - Koelen: binnentemp. 27 °CDB, 19,0 °CNB, buitentemp. 35 °CDB; equivalente leidinglengte: 7,5m"]
["","","","","","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 7,5m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 7,5m"]
["","","","","","(3) - Bevat gefluoreerde broeikasgassen","(3) - Bevat gefluoreerde broeikasgassen"]
["Leidingaansluitingen","Niveauverschil:","IU - IU","Max.","m","","7.5"]
["","","IU - OU","Max.","m","","15"]
["","Bijkomende koelmiddelvulling","","","kg/m","","0,02 (voor leidinglengte van meer dan 30 m)"]
["","Totale leidinglengte","Systeem","Werkelijk","m","","75"]
["Compressor","Type","","","","","Hermetisch gesloten swingcompressor"]
["Afmetingen","Unit","","Hoogte","mm","","","770"]
["","","","Breedte","mm","","","900"]
["","","","Diepte","mm","","","320"]
["Gewicht","Unit","","","kg","","","73"]
["Compressor","Type","","","","","","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°CDB","","","-10"]
["","","","Max.","°CDB","","","46"]
["","Verwarmen","Omgeving","Min.","°CWB","","","-15"]
["","","","Max.","°CWB","","","15.5"]
["Geluidsdrukniveau","Koelen","","Nom.","dBA","","","52"]
["","Verwarmen","","Nom.","dBA","","","52"]
["Koelmiddel","Type","","","","","","R-410A"]
["","Vulling","","","kg","","","2.99"]
["Koudemiddel","Vulling","","","tCO2Eq","","","6.2"]
["Koelmiddel","GWP","","","","","","2087.5"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","","","25"]
["","Bijkomende koelmiddelvulling","","","kg/m","","","0,02 (voor leidinglengte van meer dan 30 m)"]
["","Niveauverschil:","IU - OU","Max.","m","","","15"]
["","","IU - IU","Max.","m","","","7.5"]
["","Totale leidinglengte","Systeem","Werkelijk","m","","","75"]
["Standaard-accessoires","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["Voeding","Fase","","","","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","","","50"]
["","Spanning","","","V","","","230"]