{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5XXM-A"]
[]
[]
[]
[]
["","","","","","5XXM68A2V1B","5XXM90A2V1B"]
["Afmetingen","Unit","","Hoogte","mm","734","734"]
["","","","Breedte","mm","1040","1040"]
["","","","Diepte","mm","408","408"]
["Gewicht","Unit","","","kg","69.0","73.0"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°C DB","-10","-10"]
["","","","Max.","°C DB","50","50"]
["Geluidsdrukniveau","Koelen","","Nom.","dBA","48.0 (2)","52.0 (2)"]
["","Verwarmen","","Nom.","dBA","49.0 (2), 51.0 (3)","53.0 (2), 55.0 (3)"]
["Koelmiddel","Type","","","","R-32","R-32"]
["","Vulling","","","kg","2.00","2.40"]
["Koudemiddel","Vulling","","","tCO2Eq","1.35","1.62"]
["Koelmiddel","GWP","","","","675","675.0"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","25 (4) (5)","25 (5) (4)"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 30 m)","0,02 (voor leidinglengte van meer dan 30 m)"]
["","Niveauverschil:","IU - OU","Max.","m","15.0 (5)","15.0 (5)"]
["","","IU - IU","Max.","m","7.5 (5)","7.5 (5)"]
["","Totale leidinglengte","Systeem","Werkelijk","m","60","75"]
["Standaard-accessoires","Montagehandleiding","","","","1","1"]
["","Afvoerdop","","","","3","3"]
["","Aftapplug","","","","1","1"]
["","Montage verloopstuk","","","","1","1"]
["","Zakje schroeven","","","","2","2"]
["Bereik van het energierendement","","","","","A+++ ~ D","A+++ ~ D"]
["Voeding","Fase","","","","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","220-240","220-240"]
["Opmerkingen","","","","","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","(2) - For DX combination","(2) - For DX combination"]
["","","","","","(3) - For Space heating operation of CHVX07 unit","(3) - For Space heating operation of CHVX07 unit"]
["","","","","","(4) - Van één kamer","(4) - Van één kamer"]
["","","","","","(5) - For combination with FBA71/100/125 refer to installation manual","(5) - For combination with FBA71/100/125 refer to installation manual"]
["","","","","","(6) - Bevat gefluoreerde broeikasgassen","(6) - Bevat gefluoreerde broeikasgassen"]