{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":9,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1 (Archived)","ABQ100CV1 (Archived)","ABQ125CV1 (Archived)","ABQ140CV1 (Archived)"]
["Opgenomen vermogen","Verwarmen","","Nom.","kW","0.128","0.109"]
["","Koelen","","Nom.","kW","0.128","0.109"]
["Ventilator","Externe statische druk","","Hoog","Pa","90","70","150","150"]
["","","","Laag","Pa","64","45","111","92"]
["Koelcapaciteit","Totale capaciteit","","Nom.","kW","","","12.10","13.00"]
["Verwarmingscapaciteit","Totaalvermogen","","Nom.","kW","","","13.5","15.5"]
["Behuizing","Kleur","","","","","","Verzinkt plaatstaal/niet-geverfd","Verzinkt plaatstaal/niet-geverfd"]
["","Materiaal","","","","Gegalvaniseerd staal","Gegalvaniseerd staal"]
["Afmetingen","Unit","","Hoogte","mm","285","378","378","378"]
["","","","Breedte","mm","600","541","1300","1500"]
["","","","Diepte","mm","1007","1045","541","541"]
["Gewicht","Unit","","","kg","35","44","50","56"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","18.3","22.7","40.5","48.7"]
["","","","Nom.","m³/min","16.8","20.5","37","44"]
["","","Koeling","Middelhoog","m³/min","","","37","44"]
["","","","Laag","m³/min","15.4","18.3","34.8","37.9"]
["","","Verwarmen","Hoog","m³/min","18.3","22.7","40.5","48.7"]
["","","","Nom.","m³/min","16.8","20.5","37.4","43.9"]
["","","Verwarming","Middelhoog","m³/min","","","37.4","43.9"]
["","","Verwarmen","Laag","m³/min","15.4","18.3","34.8","37.9"]
["","Externe statische druk","","Nom.","Pa","77","57","128","122"]
["Geluidsvermogenniveau","Koelen","","","dBA","64","60","72","73"]
["","Verwarmen","","","dBA","64","60","72","73"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","Koeling","","Middelhoog","dBA","","","52","53"]
["","","","Laag","dBA","","36","50","50"]
["","Verwarmen","","Hoog","dBA","","41","53","55"]
["","Verwarming","","Middelhoog","dBA","","","52","53"]
["","Verwarmen","","Nom.","dBA","","38"]
["","","","Laag","dBA","","36","50","50"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","9.52","9.52","9.52","9.52"]
["","Gas","","Buitendiameter","mm","15.88","15.88","15.9","15.9"]
["","Drainage","","","","19.05","19.05"]
["Regelsystemen","IR-afstandsbediening","","","","","","ARCWLA","ARCWLA"]
["Standaard-accessoires","Montagehandleiding","","","","Montagehandleiding","Montagehandleiding"]
["","Draadloze afstandsbediening","","","","Draadloze afstandsbediening","Draadloze afstandsbediening"]
["","Dekrooster met vergrendeling","","","","Dekrooster met vergrendeling","Dekrooster met vergrendeling"]
["","Batterij","","","","Batterij","Batterij"]
["","Screw+Washer","","","","Screw+Washer","Screw+Washer"]
["","Bedieningshandleiding","","","","Bedieningshandleiding","Bedieningshandleiding"]
["Voeding","Naam","","","","V1","V1"]
["","Fase","","","","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","220-240","220-240"]