{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ADEQ71C2VEB / AZQS71B2V1B","ADEQ100C2VEB / AZQS100B8V1B","ADEQ125C2VEB / AZQS125B8V1B"]
["Koelcapaciteit","Nom.","","kW","6.80 (1)","9.50 (1)","12.1 (1)"]
["Koeling","SEER","","","5.40","5.10","4.71"]
["","Jaarlijks energieverbruik","","kWu/a","441","652","1,543"]
["","Vermogen","Pdesign","kW","6.80","9.50","12.1"]
["","Energieklasse","","","A","A"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","6.00","7.60","7.93"]
["","SCOP/A","","","3.81","3.81","3.50"]
["","Energieklasse","","","A","A"]
["","Jaarlijks energieverbruik","","kWu/a","2,205","2,793","3,167"]
["Nominaal energierendement","EER","","","","","2.27"]
["Verwarmingscapaciteit","Nom.","","kW","7.50 (2)","10.8 (2)","13.5 (2)"]
["Opmerkingen","","","","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 7,5m; hoogteverschil: 0m","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 7,5m; hoogteverschil: 0m","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 7,5m; hoogteverschil: 0m"]
["","","","","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 7,5m; hoogteverschil: 0m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 7,5m; hoogteverschil: 0m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 7,5m; hoogteverschil: 0m"]