{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":9,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C"]
[]
[]
[]
[]
["","","","","","AHQ71CV1","AHQ100CV1","AHQ125CV1","AHQ140CV1"]
["Opgenomen vermogen","Verwarmen","","Nom.","kW","0.106","0.149"]
["","Koelen","","Nom.","kW","0.106","0.149"]
["Ventilator","Externe statische druk","","Hoog","Pa","0","0","0","0"]
["","","","Laag","Pa","0","0","0","0"]
["Koelcapaciteit","Totale capaciteit","","Nom.","kW","","","12.10","13.00"]
["Verwarmingscapaciteit","Totaalvermogen","","Nom.","kW","","","13.5","15.5"]
["Behuizing","Kleur","","","","Wit","Wit","Wit","Wit"]
["","Materiaal","","","","Gegalvaniseerd staal","Gegalvaniseerd staal"]
["Afmetingen","Unit","","Hoogte","mm","260","260","260","285"]
["","","","Breedte","mm","1320","1538","1790","1900"]
["","","","Diepte","mm","634","634","634","680"]
["Gewicht","Unit","","","kg","38","45","65","70"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min","21.3","27.8","31","39"]
["","","Koeling","Middelhoog","m³/min","","","31","39"]
["","","","Laag","m³/min","18.9","24.8","27.2","28.3"]
["","","Verwarmen","Hoog","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min","21.3","27.8","30.6","39.1"]
["","","Verwarming","Middelhoog","m³/min","","","30.6","39.1"]
["","","Verwarmen","Laag","m³/min","18.9","24.8","27.2","28.3"]
["","Externe statische druk","","Nom.","Pa","0","0","0","0"]
["Geluidsvermogenniveau","Koelen","","","dBA","59","64","65","71"]
["","Verwarmen","","","dBA","62","64","65","71"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","49","52","52","56"]
["","","","Nom.","dBA","48","47"]
["","Koeling","","Middelhoog","dBA","","","50","53"]
["","","","Laag","dBA","46","46","49","46"]
["","Verwarmen","","Hoog","dBA","49","52","52","56"]
["","Verwarming","","Middelhoog","dBA","","","50","53"]
["","Verwarmen","","Nom.","dBA","48","47"]
["","","","Laag","dBA","46","46","49","46"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","9.52","9.52","9.52","9.52"]
["","Gas","","Buitendiameter","mm","15.88","15.88","15.9","15.9"]
["","Drainage","","","","19.05","19.05"]
["Regelsystemen","IR-afstandsbediening","","","","ARCWLA","ARCWLA","ARCWLA","ARCWLA"]
["","Bedrade afstandsbediening","","","","ARCWB","ARCWB"]
["Standaard-accessoires","Installation manual","","","","Installation manual","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","Wireless remote control"]
["","Battery","","","","Battery","Battery"]
["","Afvoerbuis","","","","Drain pipe","Drain pipe"]
["","Screw for wireless remote","","","","Screw for wireless remote","Screw for wireless remote"]
["","Ferrite Core","","","","Ferrite Core","Ferrite Core"]
["","Installation manual (Ferrite Core)","","","","Installation manual (Ferrite Core)","Installation manual (Ferrite Core)"]
["","Outdoor wiring diagram","","","","Outdoor wiring diagram","Outdoor wiring diagram"]
["","Operation manual","","","","Operation manual","Operation manual"]
["","Drain hose","","","","Drain hose","Drain hose"]
["Voeding","Naam","","","","V1","V1"]
["","Fase","","","","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","220-240","220-240"]