{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":7,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Geluidsdrukniveau","Verwarmen","","Nom.","dBA","","49.0"]
["","Koelen","","Nom.","dBA","","49.0"]
["Standaard-accessoires","Aftapplug","","","","","1"]
["","Montagehandleiding","","","","","1"]
["","Tabel koelmiddelvulling","","","","","1"]
["","Meertalige labels gefluoreerde broeikasgassen","","","","","1"]
["","Algemene voorzorgsmaatregelen","","","","","1"]
["Koelmiddel","Charge","","","TCO2Eq","","0.52"]
["","GWP","","","","","675"]
["","Vulling","","","kg","","0.76"]
["","Type","","","","","R-32"]
["Werkbereik","Koelen","Omgeving","Max.","°CDB","","50 (4), 46 (5)"]
["","","","Min.","°CDB","","-10"]
["Leidingaansluitingen","Niveauverschil:","IU - OU","Max.","m","","15"]
["","Bijkomende koelmiddelvulling","","","kg/m","","0,02 (voor leidinglengte van meer dan 10 m)"]
["Compressor","Type","","","","","Hermetisch gesloten swingcompressor"]
["Afmetingen","Unit","","Breedte","mm","","840"]
["","","","Diepte","mm","","350"]
["","","","Hoogte","mm","","552"]
["Gewicht","Unit","","","kg","","32"]
["Power supply","Fase","","","","","1~"]
["","Frequentie","","","Hz","","50"]
["","Spanning","","","V","","220-240"]
["Opmerkingen","","","","","(1) - Alleen mogelijk in combinatie met ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Bevat gefluoreerde broeikasgassen"]
["","","","","","(2) - Alleen mogelijk in combinatie met ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","","(3) - Voor elektrische gegevens zie afzonderlijke tekening"]
["","","","","","","(4) - Alleen mogelijk in combinatie met ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Alleen mogelijk in combinatie met ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Afmetingen","Unit","","Hoogte","mm","552"]
["","","","Breedte","mm","840"]
["","","","Diepte","mm","350"]
["Gewicht","Unit","","","kg","32"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°CDB","-10"]
["","","","Max.","°CDB","50 (4), 46 (5)"]
["Geluidsdrukniveau","Koelen","","Nom.","dBA","46.0"]
["","Verwarmen","","Nom.","dBA","47.0"]
["Koelmiddel","Type","","","","R-32"]
["","Vulling","","","kg","0.76"]
["Koudemiddel","Vulling","","","tCO2Eq","0.52"]
["Koelmiddel","GWP","","","","675"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","20"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 10 m)"]
["","Niveauverschil:","IU - OU","Max.","m","15"]
["Standaard-accessoires","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Voeding","Fase","","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]