{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L"]
[]
[]
[]
[]
["","","","","","ARXS50L2V1B","ARXS71L2V1B","ARXS25L2V1B (Archived)","ARXS35L2V1B (Archived)","ARXS60L2V1B (Archived)"]
["Geluidsdrukniveau","Verwarmen","","Hoog","dBA","","","47","48"]
["","","","Nom.","dBA","","52","","","49"]
["","Koelen","","Hoog","dBA","","","46","48"]
["","","","Nom.","dBA","","52","","","49"]
["Standaard-accessoires","Montagehandleiding","","","","","1","1","1","1"]
["","Aftapplug","","","","","1","1","1","1"]
["","Meertalige labels gefluoreerde broeikasgassen","","","","","1","1","","1"]
["","Tabel koelmiddelvulling","","","","","1","1","","1"]
["Koelmiddel","Charge","","","TCO2Eq","","","2.1","2.5"]
["","GWP","","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Vulling","","","kg","","1.70","1.0","1.2","1.50"]
["","Type","","","","","R-410A","R-410A","R-410A","R-410A"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm","","","780","780"]
["","","Verwarmen","Superlaag","tpm","","","740","740"]
["Werkbereik","Koelen","Omgeving","Max.","°CDB","","46","46","46","46"]
["","","","Min.","°CDB","","-10","10","10","-10"]
["","Verwarmen","Omgeving","Max.","°CWB","","18","18","18","18"]
["","","","Min.","°CWB","","-15","-15","-15","-15"]
["Leidingaansluitingen","Hoogteverschil","IU - OU","Max.","m","","20.0","15","15","20.0"]
["","Bijkomende koelmiddelvulling","","","kg/m","","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)"]
["Geluidsvermogenniveau","Koelen","","","dBA","","65","","","62"]
["","Verwarmen","","","dBA","","65","","","62"]
["Compressor","Type","","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Afmetingen","Unit","","Breedte","mm","","825","765","765","825"]
["","","","Diepte","mm","","300","285","285","300"]
["","","","Hoogte","mm","","735","550","550","735"]
["Gewicht","Unit","","","kg","","47","34","34","47"]
["Ventilator","Luchtdebiet","Verwarmen","Superlaag","cfm","","","904","904"]
["","","","Superlaag","m³/min","","","25.6","25.6"]
["","","Koelen","Superlaag","m³/min","","","30.1","30.1"]
["","","","Superlaag","cfm","","","1,063","1,063"]
["Power supply","Fase","","","","","1~","1~","1~","1~"]
["","Frequentie","","","Hz","","50","50","50","50"]
["","Spanning","","","V","","220-230-240","220-240","220-240","220-230-240"]
["Opmerkingen","","","","","","(1) - Bevat gefluoreerde broeikasgassen","","","(1) - Bevat gefluoreerde broeikasgassen"]
["Ventilator","Luchtdebiet","Koelen","Superlaag","m³/min","48.9"]
["","","Verwarmen","Superlaag","m³/min","43.1"]
["","","","Superlaag","cfm","1727"]
["","","Verwarmen","Superlaag","cfm","1522"]
["Afmetingen","Unit","","Hoogte","mm","735"]
["","","","Breedte","mm","825"]
["","","","Diepte","mm","300"]
["Gewicht","Unit","","","kg","47"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm","670"]
["","","Verwarmen","Superlaag","tpm","670"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°CDB","10"]
["","","","Max.","°CDB","46"]
["","Verwarmen","Omgeving","Min.","°CWB","-15"]
["","","","Max.","°CWB","18"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","48"]
["","Verwarmen","","Hoog","dBA","48"]
["Koelmiddel","Type","","","","R-410A"]
["","Vulling","","","kg","1.7"]
["Koudemiddel","Vulling","","","tCO2Eq","3.5"]
["Koelmiddel","GWP","","","","2087.5"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","30"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 10 m)"]
["","Niveauverschil:","IU - OU","Max.","m","20"]
["Standaard-accessoires","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["Voeding","Fase","","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]
["Opmerkingen","","","","","(1) - 220V","","(1) - Wanneer aangesloten op een multisysteem buitenunit, raadpleeg dan de karakteristieken van de multibuitenunit die aangesloten moet worden.","(1) - Wanneer aangesloten op een multisysteem buitenunit, raadpleeg dan de karakteristieken van de multibuitenunit die aangesloten moet worden."]
["","","","","","(2) - 230V","","(2) - 220V","(2) - 220V"]
["","","","","","(3) - 240V","","(3) - 230V","(3) - 230V"]
["","","","","","","","(4) - 240V","(4) - 240V"]
["","","","","","","","(5) - Bevat gefluoreerde broeikasgassen","(5) - Bevat gefluoreerde broeikasgassen"]