{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Geluidsdrukniveau","Verwarmen","","Hoog","dBA","","48"]
["","","","Laag","dBA","","45"]
["Standaard-accessoires","1","","","","","550"]
["Koelmiddel","Vulling","","","kg","","2.5"]
["","Type","","","","","1.2"]
["Ventilator","Luchtdebiet","Koelen","Superlaag","m³/min","","30.1"]
["","","","Superlaag","cfm","","1,063"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm_","","740"]
["","","Verwarmen","Superlaag","tpm_","","-15"]
["Werkbereik","Verwarmen","Omgeving","Min.","°CWB","","20"]
["","","","Max.","°CWB","","10"]
["Geluidsdrukniveau","Koelen","","Laag","dBA","","44"]
["","","","Hoog","dBA","","48"]
["Compressor","Type","","","","","Hermetisch gesloten swingcompressor"]
["Afmetingen","Unit","","Breedte","mm","","285"]
["","","","Diepte","mm","","612"]
["","","","Hoogte","mm","","765"]
["Gewicht","Unit","","","kg","","34"]
["Ventilator","Luchtdebiet","Verwarmen","Superlaag","cfm","","904"]
["","","","Superlaag","m³/min","","25.6"]
["Power supply","Fase","","","","","1~"]
["","Frequentie","","","Hz","","50"]
["","Spanning","","","V","","220-240"]
["Opmerkingen","","","","","(1) - 220V","(1) - Bevat gefluoreerde broeikasgassen"]
["","","","","","(2) - 230V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 230V"]
["","","","","","","(4) - 240V"]
["Ventilator","Luchtdebiet","Koelen","Superlaag","m³/min","30.1"]
["","","Verwarmen","Superlaag","m³/min","25.6"]
["","","","Superlaag","cfm","1063"]
["","","Verwarmen","Superlaag","cfm","904"]
["Afmetingen","Unit","","Hoogte","mm","550"]
["","","","Breedte","mm","765"]
["","","","Diepte","mm","285"]
["Gewicht","Unit","","","kg","34"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm_","780"]
["","","Verwarmen","Superlaag","tpm_","740"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°CDB","10"]
["","","","Max.","°CDB","46"]
["","Verwarmen","Omgeving","Min.","°CWB","-15"]
["","","","Max.","°CWB","18"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","46"]
["","Verwarmen","","Hoog","dBA","47"]
["","","","Laag","dBA","44"]
["Koelmiddel","Type","","","","R-410A"]
["","Vulling","","","kg","1.0"]
["Koudemiddel","Vulling","","","tCO2Eq","2.1"]
["Koelmiddel","GWP","","","","2087.5"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","20"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 10 m)"]
["","Niveauverschil:","IU - OU","Max.","m","15"]
["Standaard-accessoires","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["Voeding","Fase","","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]