{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A / ARXF-F"]
[]
[]
[]
[]
["","","","","ATXF50A2V1B / ARXF50F5V1B"]
["Buitenunit","","","","ARXF50F5V1B"]
["Koelcapaciteit","Min.","","kW","1.3"]
["","Nom.","","kW","5"]
["","Max.","","kW","5.3"]
["Verwarmingscapaciteit","Min.","","kW","1.43"]
["","Nom.","","kW","5.4"]
["","Max.","","kW","6.13"]
["Nominaal rendement","EER","","","3.27"]
["","COP","","","3.71"]
["","Jaarlijks energieverbruik","","kWh","271"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A"]
["","","Verwarming","","A"]
["Koeling","Energieklasse","","","A++"]
["","Vermogen","Pdesign","kW","5"]
["","SEER","","","6.45"]
["","Jaarlijks energieverbruik","","kWu/a","271"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A+"]
["","Vermogen","Pdesign","kW","3.8"]
["","SCOP/A","","","4.07"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","3.24"]
["","Jaarlijks energieverbruik","","kWu/a","1309"]
["Bereik van het energierendement","","","","A+++ ~ D"]
["Opmerkingen","","","","(1) - Nominale koelcapaciteiten gebaseerd op: binnentemperatuur: 27°CDB, 19°CNB; buitentemperatuur: 35°CDB, equiv. koelmiddelleidinglengte: 5m, niveauverschil: 0m. Gegevens voor reeks met hoog rendement, Eurovent-gecertificeerd"]
["","","","","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB; buitentemperatuur: 7°CDB, 6°CNB; equiv. koelmiddelleidinglengte: 5m, niveauverschil: 0m. Gegevens voor reeks met standaardrendement"]
["","","","","(3) - Voor elektrische gegevens zie afzonderlijke tekening"]