{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":87,"n_cols":11,"rows_kept":87,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A"]
[]
[]
[]
[]
["","","","","","ATXF20A5V1B","ATXF50A2V1B","ATXF60A2V1B","ATXF71A2V1B","ATXF25A5V1B (Archived)","ATXF35A5V1B (Archived)"]
["Geluidsdrukniveau","Verwarmen","","Hoog","dBA","40","42","44","45"]
["","","","Middelhoog","dBA","34","38","40","41"]
["","","","Fluisterstille werking","dBA","21","30","32","33"]
["","","","Laag","dBA","28","33","35","36"]
["","Koelen","","Middelhoog","dBA","33","39","41","42"]
["","","","Fluisterstille werking","dBA","20","31","33","34"]
["","","","Laag","dBA","26","34","36","37"]
["","","","Hoog","dBA","40","43","45","46"]
["Standaard-accessoires","Montagehandleiding","","","","1","1","1","1"]
["","Bedieningshandleiding","","","","1","1","1","1"]
["","Infrarood-afstandsbediening","","","","1","1","1","1"]
["","AAA drogecelbatterij","","","","2","2","2","2"]
["","Afstandsbedieningshouder","","","","1","1","1","1"]
["","Montageplaat","","","","1","1","1","1"]
["","Montageschroeven binnenunit","","","","2","2","2","2"]
["Besturingssystemen","Wired remote control","","","","BRC944B2, BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","6.35","6.35","6.35"]
["","Gas","","Buitendiameter","mm","9.50","12.7","12.7","12.7"]
["","Afvoer","","","","18","18","18","18"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.019","0.029","0.032","0.032"]
["","Verwarmen","","Nom.","kW","0.020","0.032","0.035","0.035"]
["Sound power level","Koelen","","","dBA","55","59","60","62"]
["","Verwarmen","","","dBA","55","61","62","62"]
["Afmetingen","Unit","","Breedte","mm","770","990","990","990"]
["","","","Diepte","mm","225","263","263","263"]
["","","","Hoogte","mm","286","295","295","295"]
["Behuizing","Kleur","","","","Wit","Wit","Wit","Wit"]
["Gewicht","Unit","","","kg","8.50","13.5","13.5","13.5"]
["Ventilator","Luchtdebiet","Verwarmen","Hoog","m³/min","10.3","17.3","17.9","17.9"]
["","","","Laag","m³/min","6.7","12.2","12.8","12.8"]
["","","","Middelhoog","m³/min","8.6","14.8","15.8","15.8"]
["","","","Fluisterstille werking","m³/min","5.3","10.7","11.3","11.3"]
["","","Koelen","Laag","m³/min","6.1","11.9","12.2","12.2"]
["","","","Middelhoog","m³/min","8.1","14.4","14.8","14.8"]
["","","","Hoog","m³/min","10.1","16.8","17.3","17.3"]
["","","","Fluisterstille werking","m³/min","4.4","10.5","10.7","10.7"]
["Power supply","Fase","","","","1~","1~","1~","1~"]
["","Frequentie","","","Hz","50","50","50","50"]
["","Naam","","","","","V1","V1","V1"]
["","Spanning","","","V","220-240","220-240","220-240","220-240"]
["Opgenomen vermogen","Koelen","","Nom.","kW","","","","","0.019","0.032"]
["","Verwarmen","","Nom.","kW","","","","","0.02","0.032"]
["Behuizing","Kleur","","","","","","","","Wit","Wit"]
["Afmetingen","Unit","","Hoogte","mm","","","","","286","286"]
["","","","Breedte","mm","","","","","770","770"]
["","","","Diepte","mm","","","","","225","225"]
["Gewicht","Unit","","","kg","","","","","8.5","9"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","","","","","10.1","11.5"]
["","","Koeling","Middelhoog","m³/min","","","","","8.1","8.3"]
["","","","Laag","m³/min","","","","","6.1","6.3"]
["","","","Fluisterstille werking","m³/min","","","","","4.4","4.5"]
["","","Verwarmen","Hoog","m³/min","","","","","10.3","11.5"]
["","","Verwarming","Middelhoog","m³/min","","","","","8.6","9"]
["","","Verwarmen","Laag","m³/min","","","","","6.7","7"]
["","","","Fluisterstille werking","m³/min","","","","","5.3","5.3"]
["Geluidsvermogenniveau","Koelen","","","dBA","","","","","55","58"]
["","Verwarmen","","","dBA","","","","","55","58"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","","","","","40","43"]
["","Koeling","","Middelhoog","dBA","","","","","33","34"]
["","","","Laag","dBA","","","","","26","27"]
["","","","Fluisterstille werking","dBA","","","","","20","20"]
["","Verwarmen","","Hoog","dBA","","","","","40","40"]
["","Verwarming","","Middelhoog","dBA","","","","","34","35"]
["","Verwarmen","","Laag","dBA","","","","","28","29"]
["","","","Fluisterstille werking","dBA","","","","","21","21"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","","","","","6.35","6.35"]
["","Gas","","Buitendiameter","mm","","","","","9.5","9.5"]
["","Drainage","","","","","","","","18","18"]
["Regelsystemen","IR-afstandsbediening","","","","","","","","ARC470A1","ARC470A1"]
["","Bedrade afstandsbediening","","","","","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standaard-accessoires","Installation manual","","","","","","","","1","1"]
["","AAA dry-cell batteries","","","","","","","","2","2"]
["","Operation manual","","","","","","","","1","1"]
["","Indoor unit fixing screws","","","","","","","","2","2"]
["","Infrared remote control","","","","","","","","1","1"]
["","Mounting plate","","","","","","","","1","1"]
["","Remote control holder","","","","","","","","1","1"]
["Voeding","Fase","","","","","","","","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","","","","","50","50"]
["","Spanning","","","V","","","","","220-240","220-240"]