{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":80,"n_cols":9,"rows_kept":80,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-C"]
[]
[]
[]
[]
["","","","","","ATXF20C5V1B","ATXF25C5V1B","ATXF42C5V1B","ATXF35C5V1B (Archived)"]
["Geluidsdrukniveau","Verwarmen","","Hoog","dBA","39.0","40.0","44.0"]
["","","","Middelhoog","dBA","34.0","34.0","34.0"]
["","","","Fluisterstille werking","dBA","21.0","21.0","22.0"]
["","","","Laag","dBA","28.0","28.0","28.0"]
["","Koelen","","Middelhoog","dBA","33.0","33.0","36.0"]
["","","","Fluisterstille werking","dBA","20.0","20.0","22.0"]
["","","","Laag","dBA","25.0","26.0","30.0"]
["","","","Hoog","dBA","39.0","40.0","45.0"]
["Standaard-accessoires","Montagehandleiding","","","","1","1","1"]
["","Bedieningshandleiding","","","","1","1","1"]
["","Batterijen","","","","1","1","1"]
["","Infrarood-afstandsbediening","","","","1","1","1"]
["","AAA drogecelbatterij","","","","2","2","2"]
["","Afstandsbedieningshouder","","","","1","1","1"]
["","Montageplaat","","","","1","1","1"]
["","Montageschroeven binnenunit","","","","2","2","2"]
["Besturingssystemen","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","6.35","6.35"]
["","Gas","","Buitendiameter","mm","9.50","9.50","9.50"]
["","Afvoer","","","","18","18","18"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.023","0.023","0.040"]
["","Verwarmen","","Nom.","kW","0.023","0.023","0.040"]
["Sound power level","Koelen","","","dBA","53.0","54.0","59.0"]
["","Verwarmen","","","dBA","55.0","55.0","59.0"]
["Afmetingen","Unit","","Breedte","mm","770","770","770"]
["","","","Diepte","mm","225","225","225"]
["","","","Hoogte","mm","286","286","286"]
["Behuizing","Kleur","","","","Wit","Wit","Wit"]
["Gewicht","Unit","","","kg","8.00","8.00","9.00"]
["Power supply","Fase","","","","1~","1~","1~"]
["","Frequentie","","","Hz","50","50","50"]
["","Spanning","","","V","220-440","220-440","220-440"]
["Opgenomen vermogen","Koelen","","Nom.","kW","","","","0.029"]
["","Verwarmen","","Nom.","kW","","","","0.029"]
["Behuizing","Kleur","","","","","","","Wit"]
["Afmetingen","Unit","","Hoogte","mm","","","","286"]
["","","","Breedte","mm","","","","770"]
["","","","Diepte","mm","","","","225"]
["Gewicht","Unit","","","kg","","","","8.5"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","","","","11.8"]
["","","Koeling","Middelhoog","m³/min","","","","8"]
["","","","Laag","m³/min","","","","6.4"]
["","","","Fluisterstille werking","m³/min","","","","4.4"]
["","","Verwarmen","Hoog","m³/min","","","","11.9"]
["","","Verwarming","Middelhoog","m³/min","","","","8.6"]
["","","Verwarmen","Laag","m³/min","","","","6.5"]
["","","","Fluisterstille werking","m³/min","","","","5.3"]
["Geluidsvermogenniveau","Koelen","","","dBA","","","","54"]
["","Verwarmen","","","dBA","","","","56"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","","","","43"]
["","Koeling","","Middelhoog","dBA","","","","34"]
["","","","Laag","dBA","","","","27"]
["","","","Fluisterstille werking","dBA","","","","20"]
["","Verwarmen","","Hoog","dBA","","","","40"]
["","Verwarming","","Middelhoog","dBA","","","","35"]
["","Verwarmen","","Laag","dBA","","","","29"]
["","","","Fluisterstille werking","dBA","","","","21"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","","","","6.35"]
["","Gas","","Buitendiameter","mm","","","","9.5"]
["","Drainage","","","","","","","18"]
["Regelsystemen","IR-afstandsbediening","","","","","","","ARC470A1"]
["","Bedrade afstandsbediening","","","","","","","BRC073A1"]
["Standaard-accessoires","Installation manual","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","Operation manual","","","","","","","1"]
["","Batteries","","","","","","","1"]
["","Indoor unit fixing screws","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Mounting plate","","","","","","","1"]
["","Remote control holder","","","","","","","1"]
["Voeding","Fase","","","","","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","","","","50"]
["","Spanning","","","V","","","","220-440"]