{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-F"]
[]
[]
[]
[]
["","","","","","ATXF50F5V1B"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.04"]
["","Verwarmen","","Nom.","kW","0.04"]
["Behuizing","Kleur","","","","Wit"]
["Afmetingen","Unit","","Hoogte","mm","286"]
["","","","Breedte","mm","770"]
["","","","Diepte","mm","225"]
["Gewicht","Unit","","","kg","9"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","12.6"]
["","","Koeling","Middelhoog","m³/min","9"]
["","","","Laag","m³/min","7.2"]
["","","","Fluisterstille werking","m³/min","6.4"]
["","","Verwarmen","Hoog","m³/min","12.8"]
["","","Verwarming","Middelhoog","m³/min","9.6"]
["","","Verwarmen","Laag","m³/min","7.2"]
["","","","Fluisterstille werking","m³/min","6.4"]
["Geluidsvermogenniveau","Koelen","","","dBA","59"]
["","Verwarmen","","","dBA","59"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","45"]
["","Koeling","","Middelhoog","dBA","39"]
["","","","Laag","dBA","34"]
["","","","Fluisterstille werking","dBA","31"]
["","Verwarmen","","Hoog","dBA","44"]
["","Verwarming","","Middelhoog","dBA","38"]
["","Verwarmen","","Laag","dBA","33"]
["","","","Fluisterstille werking","dBA","30"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6"]
["","Gas","","Buitendiameter","mm","12.7"]
["","Drainage","","","","18"]
["Regelsystemen","IR-afstandsbediening","","","","ARC480A93"]
["","Bedrade afstandsbediening","","","","BRC073A1"]
["Standaard-accessoires","ATXF50F5V1B","","","","1"]
["","Installation manual","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Voeding","Fase","","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-440"]
["Opmerkingen","","","","","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m (horizontaal)"]
["","","","","","(3) - Voor elektrische gegevens zie afzonderlijke tekening"]