{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":8,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AZAS-MY1"]
[]
[]
[]
[]
["","","","","","AZAS100M7Y1B","AZAS125M7Y1B","AZAS140M7Y1B"]
["Afmetingen","Unit","","Hoogte","mm","990","990","990"]
["","","","Breedte","mm","940","940","940"]
["","","","Diepte","mm","320","320","320"]
["Gewicht","Unit","","","kg","","70"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Werkingsbereik-=-Koelen","Werkingsbereik-=-Koelen-=- ","Werkingsbereik-=-Koelen-=- -=-Min.-=-°CDB","°CDB","","-5"]
["","","","Werkingsbereik-=-Koelen-=- -=-Max.-=-°CDB","°CDB","","46"]
["","Verwarmen","Werkingsbereik-=-Verwarmen-=- ","Werkingsbereik-=-Verwarmen-=- -=-Min.-=-°CWB","°CWB","","-15"]
["","","","Werkingsbereik-=-Verwarmen-=- -=-Max.-=-°CWB","°CWB","","15.5"]
["Geluidsvermogenniveau","Koelen","","","dBA","70","71","73"]
["","Verwarmen","","","dBA","","71","73 (1)"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Nom.-=-dB(A)","dBA","","53"]
["","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Nom.-=-dB(A)","dBA","","57"]
["Koelmiddel","Type","","","","R-32","R-32","R-32"]
["Koudemiddel","Koudemiddel-=-Inhoud-=-kg","","","kg","","2.60"]
["Koelmiddel","GWP","","","","","675"]
["Koudemiddel","Vulling","","","tCO2Eq","1.76","1.76","1.96"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","9.52","9.52","9.52"]
["Leidingaansluitingen","Gas","","Buitendiameter","mm","","15.9"]
["Koelleidingmaten","Koelleidingmaten-=-Leidinglengte","Koelleidingmaten-=-Leidinglengte-=- ","Koelleidingmaten-=-Leidinglengte-=- -=-Max.-=-m","m","","30"]
["","","Koelleidingmaten-=-Leidinglengte-=-Systeem","Koelleidingmaten-=-Leidinglengte-=-Systeem-=-Equivalent-=-m","m","","50"]
["","","Koelleidingmaten-=-Leidinglengte-=-Voorgevuld tot","Koelleidingmaten-=-Leidinglengte-=-Voorgevuld tot-=- -=-m","m","","30"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","Zie installatiehandleiding","Zie installatiehandleiding","Zie installatiehandleiding"]
["Koelleidingmaten","Koelleidingmaten-=-Hoogteverschil","Koelleidingmaten-=-Hoogteverschil-=- ","Koelleidingmaten-=-Hoogteverschil-=- -=-Max.-=-m","m","","30.0"]
["","","Koelleidingmaten-=-Hoogteverschil-=-IU - IU","Koelleidingmaten-=-Hoogteverschil-=-IU - IU-=-Max.-=-m","m","","0.5"]
["Standaard-accessoires","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["Voeding","Fase","","","","3~","3~","3~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie","","Spanningsvorm-=-Frequentie-=-Hz","","","50"]
["","Spanningsvorm-=-Spanning","","Spanningsvorm-=-Spanning-=-V","","","380-415"]
["Stroom - 50Hz","Stroom - 50Hz-=-Afzekerwaarde","","Stroom - 50Hz-=-Afzekerwaarde-=-A","","","16"]
["Opmerkingen","","","","","","(1) - Conversiewaarde echoloze kamer, gemeten volgens de JIS parameters en criteria. Deze waarden liggen iets hoger in bedrijf omwille van de omgevingscondities.","(1) - Conversiewaarde echoloze kamer, gemeten volgens de JIS parameters en criteria. Deze waarden liggen iets hoger in bedrijf omwille van de omgevingscondities."]
["Gewicht","Unit","","","kg","70","","77"]
["Werkbereik","Koelen","Omgeving","Min.","°CDB","-5","","-5"]
["","","","Max.","°CDB","46","","46"]
["","Verwarmen","Omgeving","Min.","°CWB","-15","","-15"]
["","","","Max.","°CWB","15.5","","15.5"]
["Geluidsdrukniveau","Koelen","","Nom.","dBA","53","","54"]
["","Verwarmen","","Nom.","dBA","57","","57"]
["Koelmiddel","Vulling","","","kg","2.60","","2.90"]
["","GWP","","","","675","","675"]
["Leidingaansluitingen","Gas","","Buitendiameter","mm","15.9","","15.9"]
["","Leidinglengte","Max.","OU - IU","m","30","","30"]
["","","Systeem","Equivalent","m","50","","50"]
["","","","Zonder lading","m","30","","30"]
["","Niveauverschil:","IU - OU","Max.","m","30.0","","30.0"]
["","","IU - IU","Max.","m","0.5","","0.5"]
["Spanningsvoeding","Frequentie","","","Hz","50","","50"]
["","Spanning","","","V","380-415","","380-415"]
["Stroom: 50 Hz","Maximaal zekeringamperage (MFA)","","","A","16","","16"]