{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BR00000676"]
[]
[]
[]
[]
["","","","","","BR00000676."]
["Type","","","","","Luchtreiniger"]
["Toepassing","","","","","Vloermodel"]
["Capaciteit","m³/min","","","","33.33"]
["Behuizing","Kleur","","","","Afgewerkt met gelakte, gegalvaniseerde staalplaat"]
["Afmetingen","Unit","","Hoogte","mm","1628"]
["","","","Breedte","mm","720"]
["","","","Diepte","mm","770"]
["Gewicht","Unit","","","kg","150"]
["Geschikt voor vloeroppervlakte","m²","","","","133"]
["Werking luchtreiniging","Opgenomen vermogen","","H","kW","0.379"]
["Geluidsdrukniveau","Werking luchtreiniging","","Hoog","dBA","55.9"]
["Ventilator","Luchtdebiet","Werking luchtreiniging","Turbo","m³/u","2300"]
["","","","Hoog","m³/u","2000"]
["Stofvangmethode","","","","","RedPleat-koolstof, 592x592x45 C, H14 HEPA-filtratie"]
["Bacterie-filtermethode","","","","","Astrocel III HEPA H14, A39A05C9S2R1"]
["Veiligheidsvoorzieningen","Onderdeel","","01","","Veiligheidsschakelaar (werking stopt wanneer het achterpaneel wordt geopend)"]
["Standaard-accessoires","Prefilter selected","","","","1"]
["","HEPA filter selected","","","","1"]
["","Quick Start and Maintenance Guide","","","","1"]
["","Installation and Operation Manual available for download","","","","1"]
["Voedingskabel","m","","","","3"]
["Voeding","Fase","","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50/60"]
["","Spanning","","","V","230"]
["Bedrijfsstroom","Werking luchtreiniging","","Hoog","A","1.73"]