{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1E53A"]
[]
[]
[]
[]
["","","","","BRC1E53A7"]
["Behuizing","Colour","","","Zuiver wit"]
["","Deksel knop","","","Nee"]
["","Bedrijf-LED","Kleur","","Groen"]
["Afmetingen","Unit","Hoogte","mm","120"]
["","","Breedte","mm","120"]
["","","Diepte","mm","19"]
["","Verpakte unit","Hoogte","mm","55"]
["","","Breedte","mm","160"]
["","","Diepte","mm","150"]
["Gewicht","Unit","","kg","0.200"]
["","Verpakte unit","","kg","0.415"]
["Verpakking","Materiaal","","","Karton_"]
["","Gewicht","","kg","0.05"]
["LCD","Type","","","Full dot (160 x 255)"]
["","Afmetingen","Hoogte","mm","43.2"]
["","","Breedte","mm","68.85"]
["","Achtergrondverlichting","Kleur","","Wit"]
["Omgevingstemperatuur","Bedrijf","Min.","°C","-10"]
["","","Max.","°C","50"]
["","Bewaring","Min.","°C","-20"]
["","","Max.","°C","70"]
["","Relatieve vochtigheid <","","%","95"]
["Draadaansluitingen","Lengte bedrading","Max.","m","500"]
["Back-up voor stroomuitval","","","","Ja (De klok zal blijven werken gedurende max. 48 uur)"]