{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1H52W"]
[]
[]
[]
[]
["","","","","BRC1H52W."]
["Verpakking","Materiaal","","","Karton"]
["","Gewicht","","kg","0.0850"]
["Omgevingstemperatuur","Relatieve vochtigheid <","","%","95"]
["","Bewaring","Min.","°C","-20"]
["","","Max.","°C","70"]
["","Bedrijf","Min.","°C","-10"]
["","","Max.","°C","50"]
["Afmetingen","Verpakte unit","Breedte","mm","217"]
["","","Hoogte","mm","50"]
["","","Diepte","mm","161"]
["","Unit","Breedte","mm","85"]
["","","Diepte","mm","25"]
["","","Hoogte","mm","85"]
["Behuizing","Deksel knop","","","Nee"]
["","Kleur","","","Wit"]
["","Bedrijf-LED","Kleur","","Blue status indicator"]
["LCD","Type","","","100 x 150 dots"]
["","Achtergrondverlichting","Kleur","","Wit"]
["","Afmetingen","Breedte","mm","28.0"]
["","","Hoogte","mm","40.7"]
["Gewicht","Verpakte unit","","kg","0.317"]
["","Unit","","kg","0.110"]
["Draadaansluitingen","Lengte bedrading","Max.","m","500"]