{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 3MXM-A"]
[]
[]
[]
[]
["","","","","","CHYHBH05AFV32 / 3MXM52A2V1B","CHYHBH05AAV32 / 3MXM52A2V1B","CHYHBH05AFV32 / 3MXM68A2V1B","CHYHBH05AAV32 / 3MXM68A2V1B"]
["Sanitair warm water","Algemeen","","Aangegevens belastingprofiel","","XL","","XL"]
["","Gematigd klimaat","","Energierendementsklasse waterverwarming","","A","","A"]
["COP","","","","","4.49 (1)","4.49 (1)","3.91 (1)","3.91 (1)"]
["Verwarming","Wateruitlaat gematigd klimaat 55°C","Algemeen","Seasonal space heating eff. class","","A+","","A+"]
["","","","ηs (seizoensefficiëntie ruimteverwarming)","%","111.4","","113.3"]
["","","","SCOP","","2.86","","2.91"]
["Verwarmingscapaciteit","Nom.","","","kW","4.41 (1)","","4.50 (1)"]
["Opmerkingen","","","","","(1) - DB/NB 7°C/6°C: uitgaand water condensor 35°C (DT=5°C), boiler overbrugd","(1) - DB/NB 7°C/6°C: uitgaand water condensor 35°C (DT=5°C), boiler overbrugd","(1) - DB/NB 7°C/6°C: uitgaand water condensor 35°C (DT=5°C), boiler overbrugd","(1) - DB/NB 7°C/6°C: uitgaand water condensor 35°C (DT=5°C), boiler overbrugd"]
["Verwarmingscapaciteit","Nom.","","","kW","","4.41 (1)","","4.5 (1)"]
["Verwarming van sanitair warm water","Algemeen","","Aangegevens belastingprofiel","","","XL","","XL"]
["","Gematigd klimaat","","Energierendementsklasse waterverwarming","","","A","","A"]
["Verwarming","Wateruitlaat gematigd klimaat 55°C","Algemeen","SCOP","","","2.86","","2.91"]
["","","","Seizoensefficiëntieklasse verwarming","","","A+","","A+"]