{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":7,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B (Archived)","CTXM15R5V1B (Archived)"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.029","0.029"]
["","Verwarmen","","Nom.","kW","0.023","0.023"]
["Behuizing","Kleur","","","","Wit","Wit"]
["Afmetingen","Unit","","Hoogte","mm","295","295"]
["","","","Breedte","mm","778","778"]
["","","","Diepte","mm","272","272"]
["Gewicht","Unit","","","kg","10","10"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","10.5","10.5"]
["","","Koeling","Middelhoog","m³/min","7.5","7.5"]
["","","","Laag","m³/min","5.7","5.7"]
["","","","Fluisterstille werking","m³/min","4.3","4.3"]
["","","Verwarmen","Hoog","m³/min","9.3","9.3"]
["","","Verwarming","Middelhoog","m³/min","8.2","8.2"]
["","","Verwarmen","Laag","m³/min","6.2","6.2"]
["","","","Fluisterstille werking","m³/min","5.1","5.1"]
["Geluidsvermogenniveau","Koelen","","","dBA","57","57"]
["","Verwarmen","","","dBA","54","54"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","41","41"]
["","Koeling","","Middelhoog","dBA","33","33"]
["","","","Laag","dBA","25","25"]
["","","","Fluisterstille werking","dBA","19","19"]
["","Verwarmen","","Hoog","dBA","39","39"]
["","Verwarming","","Middelhoog","dBA","34","34"]
["","Verwarmen","","Laag","dBA","26","26"]
["","","","Fluisterstille werking","dBA","20","20"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","6.35"]
["","Gas","","Buitendiameter","mm","9.5","9.5"]
["","Drainage","","","","18","18"]
["Regelsystemen","IR-afstandsbediening","","","","ARC466A67","ARC466A67"]
["","Bedrade afstandsbediening","","","","BRC073A1","BRC073A1"]
["Standaard-accessoires","Montagehandleiding","","","","1","1"]
["","Draadloze afstandsbediening","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","WLAN adapter kit","","","","1","1"]
["","Bedieningshandleiding","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Montageschroeven binnenunit","","","","2","2"]
["","Montageplaat","","","","1","1"]
["","Afstandsbedieningshouder","","","","1","1"]
["Bereik van het energierendement","","","","","A+++ ~ D","A+++ ~ D"]
["Voeding","Naam","","","","V1","V1"]
["","Fase","","","","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","220-240","220-240"]
["Opmerkingen","","","","","(1) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB, 24°CWB; equivalente leidinglengte: 5m","(1) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB, 24°CWB; equivalente leidinglengte: 5m"]
["","","","","","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m"]