{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Geluidsdrukniveau","Verwarmen","","Hoog","dBA","38","","41"]
["","","","Fluisterstille werking","dBA","21","","21"]
["","","","Laag","dBA","28","","30"]
["","Koelen","","Fluisterstille werking","dBA","21","","21"]
["","","","Laag","dBA","25","","28"]
["","","","Hoog","dBA","37","","42"]
["","","","Nom.","dBA","33"]
["","Koelen","","Nom.","dBA","31","","35"]
["Standaard-accessoires","Montagehandleiding","","","","1","","1"]
["","Bedieningshandleiding","","","","1","","1"]
["","Draadloze afstandsbediening","","","","1","","1"]
["","Batterijen","","","","2","","2"]
["","Afstandsbedieningshouder","","","","1","","1"]
["","Montageplaat","","","","1","","1"]
["","Montageschroeven binnenunit","","","","2","","2"]
["","Fotokatalytisch luchtzuiveringsfilter uit titaniumapatiet","","","","2","","2"]
["Regelsystemen","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Piping connections","Vloeistof","","Buitendiameter","mm","6.35","","6.35"]
["","Gas","","Buitendiameter","mm","9.5","","9.5"]
["","Afvoer","","","","18","","18"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.040","","0.040"]
["","Verwarmen","","Nom.","kW","0.040","","0.040"]
["Geluidsvermogenniveau","Koelen","","","dBA","55","","59"]
["","Verwarmen","","","dBA","56","","58"]
["Afmetingen","Unit","","Breedte","mm","780","","780"]
["","","","Diepte","mm","215","","215"]
["","","","Hoogte","mm","289","","289"]
["Behuizing","Colour","","","","Wit","","Wit"]
["Gewicht","Unit","","","kg","8","","8"]
["Ventilator","Luchtdebiet","Verwarmen","Hoog","m³/min","","","10.1"]
["","","","Laag","m³/min","","","6.3"]
["","","","Fluisterstille werking","m³/min","","","4.3"]
["","","Koelen","Laag","m³/min","","","5.2"]
["","","","Hoog","m³/min","","","9.2"]
["","","","Fluisterstille werking","m³/min","","","3.9"]
["","","","Nom.","m³/min","","","8.1"]
["","","Koelen","Nom.","m³/min","","","7.2"]
["Power supply","Phase","","","","1~","","1~"]
["","Frequentie","","","Hz","50","","50"]
["","Naam","","","","V1","","V1"]
["","Spanning","","","V","220-240","","220-240"]
["Opmerkingen","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Opgenomen vermogen","Koelen","","Nom.","kW","","0.04","","0.040"]
["","Verwarmen","","Nom.","kW","","0.04","","0.040"]
["Behuizing","Kleur","","","","","Wit","","Wit"]
["Afmetingen","Unit","","Hoogte","mm","","289","","289"]
["","","","Breedte","mm","","780","","780"]
["","","","Diepte","mm","","215","","215"]
["Gewicht","Unit","","","kg","","8","","8.00"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","","7.9","","9.2"]
["","","Koeling","Middelhoog","m³/min","","6.3","","7.2"]
["","","","Laag","m³/min","","4.7","","5.2"]
["","","","Fluisterstille werking","m³/min","","3.9","","3.9"]
["","","Verwarmen","Hoog","m³/min","","9","","10.1"]
["","","Verwarming","Middelhoog","m³/min","","7.5","","8.1"]
["","","Verwarmen","Laag","m³/min","","6","","6.3"]
["","","","Fluisterstille werking","m³/min","","4.3","","4.3"]
["Geluidsvermogenniveau","Koelen","","","dBA","","55","","59"]
["","Verwarmen","","","dBA","","56","","58"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","","37","","42"]
["","Koeling","","Middelhoog","dBA","","31","","35"]
["","","","Laag","dBA","","25","","28"]
["","","","Fluisterstille werking","dBA","","21","","21"]
["","Verwarmen","","Hoog","dBA","","38","","41"]
["","Verwarming","","Middelhoog","dBA","","33","","36"]
["","Verwarmen","","Laag","dBA","","28","","30"]
["","","","Fluisterstille werking","dBA","","21","","21"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","","6.35","","6.35"]
["","Gas","","Buitendiameter","mm","","9.5","","9.50"]
["","Drainage","","","","","18","","18"]
["Regelsystemen","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Standaard-accessoires","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Voeding","Naam","","","","","V1","","V1"]
["","Fase","","","","","1~","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","","50","","50"]
["","Spanning","","","V","","220-240","","220-240"]