{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CVXM-A9"]
[]
[]
[]
[]
["","","","","","CVXM20A3V1B9"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.02"]
["","Verwarmen","","Nom.","kW","0.02"]
["Behuizing","Kleur","","","","Wit"]
["Afmetingen","Unit","","Hoogte","mm","600"]
["","","","Breedte","mm","750"]
["","","","Diepte","mm","238"]
["Gewicht","Unit","","","kg","17"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","8.7"]
["","","Koeling","Middelhoog","m³/min","7"]
["","","","Laag","m³/min","4.9"]
["","","","Fluisterstille werking","m³/min","4.1"]
["","","Verwarmen","Hoog","m³/min","9.2"]
["","","Verwarming","Middelhoog","m³/min","7.2"]
["","","Verwarmen","Laag","m³/min","5.6"]
["","","","Fluisterstille werking","m³/min","4.1"]
["Geluidsvermogenniveau","Koelen","","","dBA","52"]
["","Verwarmen","","","dBA","52"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","38"]
["","Koeling","","Middelhoog","dBA","32"]
["","","","Laag","dBA","25"]
["","","","Fluisterstille werking","dBA","22"]
["","Verwarmen","","Hoog","dBA","38"]
["","Verwarming","","Middelhoog","dBA","32"]
["","Verwarmen","","Laag","dBA","25"]
["","","","Fluisterstille werking","dBA","21"]
["Koelmiddel","GWP","","","","675"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.4"]
["","Gas","","Buitendiameter","mm","9.5"]
["","Drainage","","","","VP20 (I.D. 20/O.D. 26)"]
["Regelsystemen","IR-afstandsbediening","","","","ARC466A66"]
["Regelsystemen","Bedrade afstandsbediening","","","","BRC073A1"]
["Standaard-accessoires","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Voeding","Fase","","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]