{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":9,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2U30GC-A"]
[]
[]
[]
[]
["","","","","","D2U30GC015AB","D2U30GC020AB","D2U30GC015AA (Archived)","D2U30GC020AA (Archived)"]
["Warmteverlies","Noodboiler Ps","","","kW","0.0","0.0"]
["","Noodboiler","","","kWu/24u","","","1.5","1.5"]
["","Noodboiler qS","","","kW","0.0","0.0"]
["Sanitair warm water","Opgenomen warmte (thermische netto-waarde) Qnw","Nom","Max","kW","16.7","22.2","16.7","22.2"]
["","","","Min","kW","3.3","3.3","3.3","3.3"]
["","Rendement","","Min","kW","3.0","3.0","3.0","3.0"]
["","Temperatuur","","Max","°C","70","70","85","85"]
["","Opgenomen warmte (thermische netto-waarde) Qnw","Nom","Min","kW","3.0","3.0","3.0","3.0"]
["","","","Max","kW","15.0","20.0","15.0","20.0"]
["","Energierendement","","NL kenmerken (DIN4708)","","2.0","2.1","2.0","2.1"]
["Afvoergas","Temperatuur","","Max","°C","63","69","63","69"]
["","Massadebiet (G31)","","Max","kg/u","22.5","30.0","22.5","30.0"]
["Toevoerlucht","Concentrisch","","","","Ja","Ja","Ja","Ja"]
["Sanitair warm water","Algemeen","","Energierendementsklasse waterverwarming","","A","A","A","A"]
["","","","Aangegevens belastingprofiel","","L","L","L","L"]
["Afmetingen","Unit","Hoogte","Behuizing","mm","1,895","1,895","1,895","1,895"]
["Behuizing","Colour","","","","Verkeerswit (RAL9016)/Donkergrijs (RAL7011)","Verkeerswit (RAL9016)/Donkergrijs (RAL7011)","Verkeerswit (RAL9016)/Donkergrijs (RAL7011)","Verkeerswit (RAL9016)/Donkergrijs (RAL7011)"]
["Tank","Materiaal","","","","Polypropyleen","Polypropyleen","Polypropyleen","Polypropyleen"]
["Verwarming","Algemeen","","Seizoensrendementsklasse verwarming","","A","A","A","A"]
["","","","ηs (seizoensrendement van verwarming)","%","91","92","91","92"]
["Centrale verwarming","Opgenomen warmte Qn (thermische bruto-waarde)","Nom","Min","kW","3.3","3.3","3.3","3.3"]
["","","","Max","kW","16.7","22.2","16.7","22.2"]
["","Watertemperatuur","","Max","°C","85","85","90","90"]
["","Uitgaand Pn bij 80/60°C","","Min","kW","2.9","2.9","2.9","2.9"]
["","","","Nom","kW","14.6","19.5","14.6","19.5"]
["","Opgenomen warmte Qn (thermische netto-waarde)","Nom","Max","kW","15.0","20.0","15.0","20.0"]
["","","","Min","kW","3.0","3.0","3.0","3.0"]
["","Uitgaand Pn bij 50/30°C","","Min","kW","3.2","3.2","3.2","3.2"]
["","","","Nom","kW","15.7","20.9","15.7","20.9"]
["Gas","Aansluiting","","Diameter","mm","20","20","20","20"]
["","Verbruik (G31)","","Min","m³/u","0.16","0.16","0.16","0.16"]
["","","","Max","m³/u","0.62","0.82","0.62","0.82"]
["","NOx-klasse","","","","6","6","6","6"]
["Opmerkingen","","","","","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897"]