{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Omgevingstemperatuur","Relatieve vochtigheid <","","","%","85"]
["Maximaal aantal aansluitbare binnenunits","","","","","32"]
["Opgenomen vermogen","kW","","","","0.015 (1)"]
["Communicatie","DIII-NET","","Hoeveelheid","","1"]
["","","","Opmerking","","DIII-NET (F1F2)"]
["","Ethernet","","Hoeveelheid","","1"]
["","Ingangsklem","Digitaal","Hoeveelheid","","4"]
["Afmetingen","Unit","","Breedte","mm","384"]
["","","","Diepte","mm","92"]
["","","","Hoogte","mm","136"]
["Maximaal aantal aansluitbare buitenunits","","","","","7"]
["Power supply","Frequentie","","","Hz","50/60"]
["","Spanning","","","V","110-240 AC"]
["Opmerkingen","","","","","(1) - Inclusief het opgenomen vermogen van de WAGO-stroomvoorziening, de CPU-module en de I/O-module"]
["","","","","","(2) - De afmetingen zijn inclusief de WAGO-stroomvoorziening, de CPU-module, de I/O-module en de nodige vrije ruimte tussen de verschillende onderdelen."]
["","","","","","(3) - De afmetingen van het optionele scherm zijn: hoogte: 209 mm, breedte: 123 mm, diepte: 8,5 mm"]