{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCM601B51"]
[]
[]
[]
[]
["","","","","DCM601B51."]
["Omgevingstemperatuur","Relatieve vochtigheid <","","%","85"]
["","Bedrijf","Min.","°C","0"]
["","","Max.","°C","40"]
["Afmetingen","Unit","Breedte","mm","290"]
["","","Diepte","mm","50"]
["","","Hoogte","mm","243"]
["Gewicht","Unit","","kg","2.2"]
["Power supply","Frequentie","","Hz","50/60"]
["","Spanning","","V","AC 100-240"]