{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":8,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DucoBox Energy Comfort Plus"]
[]
[]
[]
[]
["","","","","","DucoBox Energy Comfort Plus D350","DucoBox Energy Comfort Plus D450","DucoBox Energy Comfort Plus D550"]
["Artikelnummer","","","","","00004704","00004705","00004706"]
["Behuizing","Materiaal","","","","Gecoat plaatstaal + EPP","Gecoat plaatstaal + EPP","Gecoat plaatstaal + EPP"]
["Afmetingen","Unit","","Hoogte","mm","803","803","803"]
["","","","Breedte","mm","760","760","760"]
["","","","Diepte","mm","584","584","584"]
["Gewicht","Unit","","","kg","47","47","47"]
["Ventilator","Luchtdebiet - 50Hz","Warmtewisselingsmodus","Ultrahoog","m³/u","350","450","550"]
["","","Bypass-modus","Ultrahoog","m³/u","350","450","550"]
["Warmtewisselingssysteem","","","","","Totale warmtewisselaar met lucht-luchtventilatie (voelbare + latente warmte) van het dwarsstroomtype","Uitwisseling voelbare warmte lucht/lucht van het dwarsstroomtype","Totale warmtewisselaar met lucht-luchtventilatie (voelbare + latente warmte) van het dwarsstroomtype"]
["Warmtewisselingselement","","","","","v1: PP - v2: PET/Alu","v1: PP - v2: PET/Alu","v1: PP - v2: PET/Alu"]
["Aansluiting kanaaldiameter","mm","","","","180","180","180"]
["Bedrijfsmodus","","","","","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus"]
["SEC-Klasse","","","","","Zie opmerking 2","Zie opmerking 2","Zie opmerking 2"]
["Maximaal debiet bij een externe statische druk van 100 Pa","Debiet","","","m³/u","350","450","550"]
["Geluidsvermogenniveau (Lwa)","dB","","","","48","49","54.0"]
["Jaarlijks elektriciteitsverbruik","kWu/a","","","","217.5 (1)","254.4 (1)","315.2 (1)"]
["Jaarlijkse besparing op verwarming","Gematigd klimaat","","","kWu/a","4547 (1)","4512 (1)","4413 (1)"]
["","Koud klimaat","","","kWu/a","8895 (1)","8826 (1)","8633 (1)"]
["","Warm klimaat","","","kWu/a","2056 (1)","2040 (1)","1996 (1)"]
["Voeding","Fase","","","","3-core power cable with earthed plug","3-core power cable with earthed plug","3-core power cable with earthed plug"]
["Spanningsvoeding","Frequentie","","","Hz","50","50","50"]
["","Spanning","","","V","230","230","230"]
["Opmerkingen","","","","","(1) - Manuele regeling (geen DCV)","(1) - Manuele regeling (geen DCV)","(1) - Manuele regeling (geen DCV)"]
["","","","","","(2) - Met 2 sensoren (regelfactor 0,65): A+; Overige: A","(2) - Met 2 sensoren (regelfactor 0,65): A+; Overige: A","(2) - Met 2 sensoren (regelfactor 0,65): A+; Overige: A"]
["","","","","","(3) - Dynamische luchtstroomfilter toevoerlucht (520 x 190 x 15 mm) Standaard: ISO 16890 Grof 65% (= G4) Optioneel: ISO 16890 ePM1 55% (=F7) Dynamische luchtstroomfilter afvoerlucht (520 x 190 x 15 mm) Standaard: ISO 16890 Grof 65% (= G4)","(3) - Dynamische luchtstroomfilter toevoerlucht (520 x 190 x 15 mm) Standaard: ISO 16890 Grof 65% (= G4) Optioneel: ISO 16890 ePM1 55% (=F7) Dynamische luchtstroomfilter afvoerlucht (520 x 190 x 15 mm) Standaard: ISO 16890 Grof 65% (= G4)","(3) - Dynamische luchtstroomfilter toevoerlucht (520 x 190 x 15 mm) Standaard: ISO 16890 Grof 65% (= G4) Optioneel: ISO 16890 ePM1 55% (=F7) Dynamische luchtstroomfilter afvoerlucht (520 x 190 x 15 mm) Standaard: ISO 16890 Grof 65% (= G4)"]