{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":21,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DucoBox Energy Premium"]
[]
[]
[]
[]
["","","","","","DucoBox Energy Premium 325 - 1ZS Left","DucoBox Energy Premium 325 - 1ZH Left","DucoBox Energy Premium 325 - 2ZS Left","DucoBox Energy Premium 325 - 2ZH Left","DucoBox Energy Premium 325 - 1ZS Right","DucoBox Energy Premium 325 - 1ZH Right","DucoBox Energy Premium 325 - 2ZS Right","DucoBox Energy Premium 325 - 2ZH Right","DucoBox Energy Premium 400 - 1ZS Left","DucoBox Energy Premium 400 - 1ZH Left","DucoBox Energy Premium 400 - 2ZS Left","DucoBox Energy Premium 400 - 2ZH Left","DucoBox Energy Premium 400 - 1ZS Right","DucoBox Energy Premium 400 - 1ZH Right","DucoBox Energy Premium 400 - 2ZS Right","DucoBox Energy Premium 400 - 2ZH Right"]
["Artikelnummer","","","","","00004358","00004360","00004362","00004364","00004359","00004361","00004363","00004365","00004366","00004368","00004370","00004372","00004367","00004369","00004371","00004373"]
["Opgenomen vermogen - 50Hz","Warmtewisselingsmodus","Nom.","Ultrahoog","kW","0.118 (1)","0.118 (1)","0.118 (1)","0.118 (1)","0.118 (1)","0.118 (1)","0.118 (1)","0.118 (1)","0.18 (1)","0.18 (1)","0.18 (1)","0.18 (1)","0.18 (1)","0.18 (1)","0.18 (1)","0.18 (1)"]
["","Bypass-modus","Nom.","Ultrahoog","kW","0.118 (1)","0.118 (1)","0.118 (1)","0.118 (1)","0.118 (1)","0.118 (1)","0.118 (1)","0.118 (1)","0.18 (1)","0.18 (1)","0.18 (1)","0.18 (1)","0.18 (1)","0.18 (1)","0.18 (1)","0.18 (1)"]
["Behuizing","Materiaal","","","","Gecoat plaatstaal","Gecoat plaatstaal","Gecoat plaatstaal","Gecoat plaatstaal","Gecoat plaatstaal","Gecoat plaatstaal","Gecoat plaatstaal","Gecoat plaatstaal","Gecoat plaatstaal","Gecoat plaatstaal","Gecoat plaatstaal","Gecoat plaatstaal","Gecoat plaatstaal","Gecoat plaatstaal","Gecoat plaatstaal","Gecoat plaatstaal"]
["Afmetingen","Unit","","Hoogte","mm","957","957","957","957","957","957","957","957","957","957","957","957","957","957","957","957"]
["","","","Breedte","mm","740","740","740","740","740","740","740","740","740","740","740","740","740","740","740","740"]
["","","","Diepte","mm","585","585","585","585","585","585","585","585","585","585","585","585","585","585","585","585"]
["Gewicht","Unit","","","kg","47","47","47","47","47","47","47","47","47","47","47","47","47","47","47","47"]
["Ventilator","Luchtdebiet - 50Hz","Warmtewisselingsmodus","Ultrahoog","m³/u","325","325","325","325","325","325","325","325","400","400","400","400","400","400","400","400"]
["","","Bypass-modus","Ultrahoog","m³/u","325","325","325","325","325","325","325","325","400","400","400","400","400","400","400","400"]
["","Externe statische druk - 50Hz","","Ultrahoog","Pa","100","100","100","100","100","100","100","100","100","100","100","100","100","100","100","100"]
["Werkbereik","Rond unit","","","°CDB","-5°C~40°CDB, 90% RH of lager","-5°C~40°CDB, 90% RH of lager","-5°C~40°CDB, 90% RH of lager","-5°C~40°CDB, 90% RH of lager","-5°C~40°CDB, 90% RH of lager","-5°C~40°CDB, 90% RH of lager","-5°C~40°CDB, 90% RH of lager","-5°C~40°CDB, 90% RH of lager","-5°C~40°CDB, 90% RH of lager","-5°C~40°CDB, 90% RH of lager","-5°C~40°CDB, 90% RH of lager","-5°C~40°CDB, 90% RH of lager","-5°C~40°CDB, 90% RH of lager","-5°C~40°CDB, 90% RH of lager","-5°C~40°CDB, 90% RH of lager","-5°C~40°CDB, 90% RH of lager"]
["Geluidsdrukniveau - 50Hz","Warmtewisselingsmodus","","Ultrahoog","dBA","52","52","52","52","52","52","52","52","52.5","52.5","52.5","52.5","52.5","52.5","52.5","52.5"]
["","Bypass-modus","","Ultrahoog","dBA","52","52","52","52","52","52","52","52","52.5","52.5","52.5","52.5","52.5","52.5","52.5","52.5"]
["Warmtewisselingssysteem","","","","","Totale warmtewisselaar met lucht-luchtventilatie (voelbare + latente warmte) van het dwarsstroomtype","Uitwisseling voelbare warmte lucht/lucht van het dwarsstroomtype","Uitwisseling voelbare warmte lucht/lucht van het dwarsstroomtype","Uitwisseling voelbare warmte lucht/lucht van het dwarsstroomtype","Uitwisseling voelbare warmte lucht/lucht van het dwarsstroomtype","Uitwisseling voelbare warmte lucht/lucht van het dwarsstroomtype","Uitwisseling voelbare warmte lucht/lucht van het dwarsstroomtype","Uitwisseling voelbare warmte lucht/lucht van het dwarsstroomtype","Totale warmtewisselaar met lucht-luchtventilatie (voelbare + latente warmte) van het dwarsstroomtype","Uitwisseling voelbare warmte lucht/lucht van het dwarsstroomtype","Uitwisseling voelbare warmte lucht/lucht van het dwarsstroomtype","Uitwisseling voelbare warmte lucht/lucht van het dwarsstroomtype","Uitwisseling voelbare warmte lucht/lucht van het dwarsstroomtype","Uitwisseling voelbare warmte lucht/lucht van het dwarsstroomtype","Uitwisseling voelbare warmte lucht/lucht van het dwarsstroomtype","Uitwisseling voelbare warmte lucht/lucht van het dwarsstroomtype"]
["Warmtewisselingselement","","","","","PET/Polystyreen","PET/Polystyreen","PET/Polystyreen","PET/Polystyreen","PET/Polystyreen","PET/Polystyreen","PET/Polystyreen","PET/Polystyreen","PET/Polystyreen","PET/Polystyreen","PET/Polystyreen","PET/Polystyreen","PET/Polystyreen","PET/Polystyreen","PET/Polystyreen","PET/Polystyreen"]
["Aansluiting kanaaldiameter","mm","","","","Interne diameter Ø160 / Externe diameter Ø190","Interne diameter Ø160 / Externe diameter Ø190","Interne diameter Ø160 / Externe diameter Ø190","Interne diameter Ø160 / Externe diameter Ø190","Interne diameter Ø160 / Externe diameter Ø190","Interne diameter Ø160 / Externe diameter Ø190","Interne diameter Ø160 / Externe diameter Ø190","Interne diameter Ø160 / Externe diameter Ø190","Interne diameter Ø160 / Externe diameter Ø190","Interne diameter Ø160 / Externe diameter Ø190","Interne diameter Ø160 / Externe diameter Ø190","Interne diameter Ø160 / Externe diameter Ø190","Interne diameter Ø160 / Externe diameter Ø190","Interne diameter Ø160 / Externe diameter Ø190","Interne diameter Ø160 / Externe diameter Ø190","Interne diameter Ø160 / Externe diameter Ø190"]
["Bedrijfsmodus","","","","","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus","Warmtewisselingsmodus, Bypass-Modus, Vorstbeschermingsmodus"]
["SEC-Klasse","","","","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["Maximaal debiet bij een externe statische druk van 100 Pa","Debiet","","","m³/u","327","327","327","327","327","327","327","327","405","405","405","405","405","405","405","405"]
["Geluidsvermogenniveau (Lwa)","dB","","","","41","41","41","41","41","41","41","41","46","46","46","46","46","46","46","46"]
["Jaarlijks elektriciteitsverbruik","kWu/a","","","","112.4","112.4","112.4","112.4","112.4","112.4","112.4","112.4","127.5","127.5","127.5","127.5","127.5","127.5","127.5","127.5"]
["Jaarlijkse besparing op verwarming","Gematigd klimaat","","","kWu/a","4673","4673","4673","4673","4673","4673","4673","4673","4652","4652","4652","4652","4652","4652","4652","4652"]
["","Koud klimaat","","","kWu/a","9141","9141","9141","9141","9141","9141","9141","9141","9100","9100","9100","9100","9100","9100","9100","9100"]
["","Warm klimaat","","","kWu/a","2113","2113","2113","2113","2113","2113","2113","2113","2104","2104","2104","2104","2104","2104","2104","2104"]
["Voeding","Fase","","","","Een-fase geaard","Een-fase geaard","Een-fase geaard","Een-fase geaard","Een-fase geaard","Een-fase geaard","Een-fase geaard","Een-fase geaard","Een-fase geaard","Een-fase geaard","Een-fase geaard","Een-fase geaard","Een-fase geaard","Een-fase geaard","Een-fase geaard","Een-fase geaard"]
["Spanningsvoeding","Frequentie","","","Hz","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50"]
["","Spanning","","","V","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230"]
["Opmerkingen","","","","","(1) - Bij max debiet","(1) - Bij max debiet","(1) - Bij max debiet","(1) - Bij max debiet","(1) - Bij max debiet","(1) - Bij max debiet","(1) - Bij max debiet","(1) - Bij max debiet","(1) - Bij max debiet","(1) - Bij max debiet","(1) - Bij max debiet","(1) - Bij max debiet","(1) - Bij max debiet","(1) - Bij max debiet","(1) - Bij max debiet","(1) - Bij max debiet"]
["","","","","","(2) - Bij 250 m3/h","(2) - Bij 250 m3/h","(2) - Bij 250 m3/h","(2) - Bij 250 m3/h","(2) - Bij 250 m3/h","(2) - Bij 250 m3/h","(2) - Bij 250 m3/h","(2) - Bij 250 m3/h","(2) - Bij 250 m3/h","(2) - Bij 250 m3/h","(2) - Bij 250 m3/h","(2) - Bij 250 m3/h","(2) - Bij 250 m3/h","(2) - Bij 250 m3/h","(2) - Bij 250 m3/h","(2) - Bij 250 m3/h"]
["","","","","","(3) - Bij 100 m3/h","(3) - Bij 100 m3/h","(3) - Bij 100 m3/h","(3) - Bij 100 m3/h","(3) - Bij 100 m3/h","(3) - Bij 100 m3/h","(3) - Bij 100 m3/h","(3) - Bij 100 m3/h","(3) - Bij 100 m3/h","(3) - Bij 100 m3/h","(3) - Bij 100 m3/h","(3) - Bij 100 m3/h","(3) - Bij 100 m3/h","(3) - Bij 100 m3/h","(3) - Bij 100 m3/h","(3) - Bij 100 m3/h"]
["","","","","","(4) - Bij 325 m3/h","(4) - Bij 325 m3/h","(4) - Bij 325 m3/h","(4) - Bij 325 m3/h","(4) - Bij 325 m3/h","(4) - Bij 325 m3/h","(4) - Bij 325 m3/h","(4) - Bij 325 m3/h","(4) - Bij 325 m3/h","(4) - Bij 325 m3/h","(4) - Bij 325 m3/h","(4) - Bij 325 m3/h","(4) - Bij 325 m3/h","(4) - Bij 325 m3/h","(4) - Bij 325 m3/h","(4) - Bij 325 m3/h"]
["","","","","","(5) - Bij 332 m3/h","(5) - Bij 332 m3/h","(5) - Bij 332 m3/h","(5) - Bij 332 m3/h","(5) - Bij 332 m3/h","(5) - Bij 332 m3/h","(5) - Bij 332 m3/h","(5) - Bij 332 m3/h","(5) - Bij 332 m3/h","(5) - Bij 332 m3/h","(5) - Bij 332 m3/h","(5) - Bij 332 m3/h","(5) - Bij 332 m3/h","(5) - Bij 332 m3/h","(5) - Bij 332 m3/h","(5) - Bij 332 m3/h"]
["","","","","","(6) - Bij 401 m3/h","(6) - Bij 401 m3/h","(6) - Bij 401 m3/h","(6) - Bij 401 m3/h","(6) - Bij 401 m3/h","(6) - Bij 401 m3/h","(6) - Bij 401 m3/h","(6) - Bij 401 m3/h","(6) - Bij 401 m3/h","(6) - Bij 401 m3/h","(6) - Bij 401 m3/h","(6) - Bij 401 m3/h","(6) - Bij 401 m3/h","(6) - Bij 401 m3/h","(6) - Bij 401 m3/h","(6) - Bij 401 m3/h"]