{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":8,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EABX-D9W7 / EPGA011-016DV7"]
[]
[]
[]
[]
["","","","","","EABX16DF9W7 / EPGA11DAV37","EABX16DF9W7 / EPGA14DAV37","EABX16DF9W7 / EPGA16DAV37"]
["COP","","","","","5.15 (1), 3.88 (2)","4.99 (1), 3.65 (2)","4.78 (1), 3.71 (2)"]
["Binnenunit","","","","","EABX16DA9W7","EABX16DA9W7","EABX16DA9W7"]
["Verwarming","Wateruitlaat gematigd klimaat 55°C","Algemeen","Seasonal space heating eff. class","","A++","A++","A++"]
["","","","ηs (seizoensefficiëntie ruimteverwarming)","%","130","132","134"]
["","","","SCOP","","3.32","3.37","3.43"]
["Koelcapaciteit","Nom.","","","kW","10.5 (1), 10.7 (2)","11.1 (1), 11.9 (2)","13.5 (1), 11.9 (2)"]
["EER","","","","","4.75 (1), 3.23 (2)","4.09 (1), 2.99 (2)","3.94 (1), 2.99 (2)"]
["Verwarmingscapaciteit","Nom.","","","kW","11.1 (1), 11.3 (2)","14.5 (1), 14.5 (2)","16.5 (1), 15.6 (2)"]
["Opgenomen vermogen","Koelen","","Nom.","kW","2.21 (1), 3.30 (2)","2.72 (1), 3.97 (2)","3.42 (1), 3.97 (2)"]
["","Verwarmen","","Nom.","kW","2.16 (1), 2.91 (2)","2.91 (1), 3.96 (2)","3.45 (1), 4.21 (2)"]
["Opmerkingen","","","","","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)"]