{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","EGSQH10S18AA9W"]
["Geluidsdrukniveau","Nom.","","","dBA","32.0 (6)"]
["Koelmiddel","GWP","","","","2,090"]
["","Vulling","","","kg","1.80"]
["","Type","","","","R-410A"]
["Bedrijfsbereik","Montageruimte","","Min.","°C","5.00"]
["","","","Max.","°C","30.0"]
["","Verwarmen","Waterzijde","Max.","°C","60.0 (7), 65.0 (8)"]
["","","","Min.","°C","24 (7), 24 (8)"]
["","Kant van glycol","","Min.","°C","-5.00"]
["","","","Max.","°C","20.0"]
["","Sanitair warm water","Waterzijde","Max.","°C","55 (7), 60 (9)"]
["","","","Min.","°C","25 (7), 25 (9)"]
["Opgenomen vermogen","Nom.","","","kW","2.38 (1), 2.89 (2)"]
["Geluidsvermogenniveau","Nom.","","","dBA","46.0"]
["COP","","","","","4.33 (1), 3.18 (2)"]
["Afmetingen","Unit","","Breedte","mm","600"]
["","","","Diepte","mm","728"]
["","","","Hoogte","mm","1,730"]
["Behuizing","Materiaal","","","","Voorgelakte metaalplaat"]
["","Colour","","","","Wit"]
["Tank","Watervolume","","","l","180"]
["","Corrosiebescherming","","","","Anode"]
["","Isolatie","","Warmteverlies","kWu/24u","1.36 (4)"]
["Gewicht","Unit","","","kg","210"]
["Verwarming","Wateruitlaat gematigd klimaat 35°C","Algemeen","ηs (seizoensefficiëntie ruimteverwarming)","%","194"]
["","","","Seizoensefficiëntieklasse verwarming","","A+++"]
["","","","SCOP","","5.06"]
["","Wateruitlaat gematigd klimaat 55°C","Algemeen","Seasonal space heating eff. class","","A++"]
["","","","ηs (seizoensefficiëntie ruimteverwarming)","%","139"]
["","","","SCOP","","3.68"]
["Verwarmingscapaciteit","Nom.","","","kW","10.3 (1), 9.20 (2)"]
["","Min.","","","kW","3.11 (1), 2.47 (2)"]
["","Max.","","","kW","13.0 (1), 11.9 (2)"]
["Power supply","Phase","","","","3~"]
["","Naam","","","","9W"]
["","Frequentie","","","Hz","50"]
["","Spanning","","","V","400"]
["Spanning","Aanbevolen zekeringen","","","A","25"]
["Opmerkingen","","","","","(1) - EWB/LWB 0°C/-3°C - LWC 35°C (DT=5°C)"]
["","","","","","(2) - EWB/LWB 0°C/-3°C - LWC 45℃ (DT=5°C)"]
["","","","","","(3) - met 40% propyleenglycol"]
["","","","","","(4) - Warmteverlies volgens EN12897"]
["","","","","","(5) - Inclusief leidingen + PHE + back-upverwarming; exclusief expansievat"]
["","","","","","(6) - Het geluidsdrukniveau wordt gemeten met een microfoon op 1 m van de unit. Het is een relatieve waarde die afhangt van de afstand en de akoestische omgeving."]
["","","","","","(7) - Met warmtepomp"]
["","","","","","(8) - Met warmtepomp + back-upverwarming"]
["","","","","","(9) - Met back-upverwarming"]