{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":10,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBX-CB / ERHQ-BW1"]
[]
[]
[]
[]
["","","","","EHBX11CB3V / ERHQ011BAW1","EHBX11CB9W / ERHQ011BAW1","EHBX16CB3V / ERHQ014BAW1","EHBX16CB9W / ERHQ014BAW1","EHBX16CB3V / ERHQ016BAW1","EHBX16CB9W / ERHQ016BAW1"]
["COP","","","","4.30 (1), 3.39 (2)","4.30 (1), 3.39 (2)","4.24 (1), 3.22 (2)","4.24 (1), 3.22 (2)","4.20 (1), 3.22 (2)","4.20 (1), 3.22 (2)"]
["Koelcapaciteit","Nom.","","kW","15.1 (1), 11.7 (2)","15.1 (1), 11.7 (2)","16.1 (1), 12.6 (2)","16.1 (1), 12.6 (2)","16.8 (1), 13.1 (2)","16.8 (1), 13.1 (2)"]
["EER","","","","3.32 (1), 2.72 (2)","3.32 (1), 2.72 (2)","2.96 (1), 2.47 (2)","2.96 (1), 2.47 (2)","2.72 (1), 2.29 (2)","2.72 (1), 2.29 (2)"]
["Verwarmingscapaciteit","Nom.","","kW","11.3 (1), 11.0 (2)","11.3 (1), 11.0 (2)","14.5 (1), 13.6 (2)","14.5 (1), 13.6 (2)","16.1 (1), 15.1 (2)","16.1 (1), 15.1 (2)"]
["Opgenomen vermogen","Koelen","Nom.","kW","4.53 (1), 4.31 (2)","4.53 (1), 4.31 (2)","5.43 (1), 5.08 (2)","5.43 (1), 5.08 (2)","6.16 (1), 5.73 (2)","6.16 (1), 5.73 (2)"]
["","Verwarmen","Nom.","kW","2.63 (1), 3.24 (2)","2.63 (1), 3.24 (2)","3.42 (1), 4.21 (2)","3.42 (1), 4.21 (2)","3.82 (1), 4.69 (2)","3.82 (1), 4.69 (2)"]
["Opmerkingen","","","","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)"]
["","","","","(3) - T. omg. 35°C – Uitgaand water verdamper (LWE) 7°C (DT = 5°C)","(3) - T. omg. 35°C – Uitgaand water verdamper (LWE) 7°C (DT = 5°C)","(3) - T. omg. 35°C – Uitgaand water verdamper (LWE) 7°C (DT = 5°C)","(3) - T. omg. 35°C – Uitgaand water verdamper (LWE) 7°C (DT = 5°C)","(3) - T. omg. 35°C – Uitgaand water verdamper (LWE) 7°C (DT = 5°C)","(3) - T. omg. 35°C – Uitgaand water verdamper (LWE) 7°C (DT = 5°C)"]
["","","","","(4) - Omgevingstemp. 35°C – Uitgaand water verdamper (LWE) 18℃ (DT = 5°C)","(4) - Omgevingstemp. 35°C – Uitgaand water verdamper (LWE) 18℃ (DT = 5°C)","(4) - Omgevingstemp. 35°C – Uitgaand water verdamper (LWE) 18℃ (DT = 5°C)","(4) - Omgevingstemp. 35°C – Uitgaand water verdamper (LWE) 18℃ (DT = 5°C)","(4) - Omgevingstemp. 35°C – Uitgaand water verdamper (LWE) 18℃ (DT = 5°C)","(4) - Omgevingstemp. 35°C – Uitgaand water verdamper (LWE) 18℃ (DT = 5°C)"]
["","","","","(5) - DB/WB 7°C/6°C - Uitgaand water condensor (LWC) 35°C(DT=5°C)","(5) - DB/WB 7°C/6°C - Uitgaand water condensor (LWC) 35°C(DT=5°C)","(5) - DB/WB 7°C/6°C - Uitgaand water condensor (LWC) 35°C(DT=5°C)","(5) - DB/WB 7°C/6°C - Uitgaand water condensor (LWC) 35°C(DT=5°C)","(5) - DB/WB 7°C/6°C - Uitgaand water condensor (LWC) 35°C(DT=5°C)","(5) - DB/WB 7°C/6°C - Uitgaand water condensor (LWC) 35°C(DT=5°C)"]
["","","","","(6) - DB/WB 7 °C / 6 °C - Uitgaand water condensor (LWC) 45℃ (Dt=5 °C)","(6) - DB/WB 7 °C / 6 °C - Uitgaand water condensor (LWC) 45℃ (Dt=5 °C)","(6) - DB/WB 7 °C / 6 °C - Uitgaand water condensor (LWC) 45℃ (Dt=5 °C)","(6) - DB/WB 7 °C / 6 °C - Uitgaand water condensor (LWC) 45℃ (Dt=5 °C)","(6) - DB/WB 7 °C / 6 °C - Uitgaand water condensor (LWC) 45℃ (Dt=5 °C)","(6) - DB/WB 7 °C / 6 °C - Uitgaand water condensor (LWC) 45℃ (Dt=5 °C)"]