{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSHB-D3"]
[]
[]
[]
[]
["","","","","","EHSHB04P30DA3","EHSHB08P30DA3","EHSHB08P50DA3"]
["Behuizing","Kleur","","","","Verkeerswit (RAL9016)/Donkergrijs (RAL7011)","Verkeerswit (RAL9016)/Donkergrijs (RAL7011)","Verkeerswit (RAL9016)/Donkergrijs (RAL7011)"]
["","Materiaal","","","","Slagvast polypropyleen","Slagvast polypropyleen","Slagvast polypropyleen"]
["Afmetingen","Unit","","Hoogte","mm","1891","1891","1896"]
["","","","Breedte","mm","595","595","790"]
["","","","Diepte","mm","615","615","790"]
["Gewicht","Unit","","","kg","76.0","76.0","99.0"]
["PED (richtlijn drukapparatuur)","Categorie","","","","art. 3,3","art. 3,3","art. 3,3"]
["Koelmiddel","Type","","","","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0"]
["","Vulling","","","kg","1.50","1.50","1.50"]
["Geluidsvermogenniveau","Nom.","","","dBA","39","39","39"]
["Werkingsbereik","Verwarmen","waterzijdig","Min.","°C","18","18","18"]
["Werkbereik","Verwarmen","Waterzijde","Max.","°C","65","65","65"]
["","Koelen","Omgeving","Min.","°CDB","10","10","10"]
["","","Waterzijde","Min.","°C","5","5","5"]
["","","","Max.","°C","22","22","22"]
["Voeding","Fase","","","","1~","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50","50"]
["","Spanning","","","V","230","230","230"]
["Elektrische verwarming","Spanningsvoeding","","Elektrische verwarming-=-Spanningsvoeding-=-Naam","","3V / 9W","3V / 9W","3V / 9W"]
["","","","Fase","","1~ / 3~","1~ / 3~","1~ / 3~"]
["","","","Frequentie","Hz","50","50","50"]
["Opmerkingen","","","","","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃"]
["","","","","","","","(5) - Verwarming van ketel alleen met warmtepomp, geen elektrische verwarming"]