{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-E / ERGA-EV7"]
[]
[]
[]
[]
["","","","","","EHSX04P30EF / ERGA04EAV37","EHSX04P50EF / ERGA04EAV37"]
["Binnenunit","","","","","EHSX04P30EF","EHSX04P50EF"]
["Verwarmingscapaciteit","Nom.","","","kW","4.36 (1), 4.60 (2)","4.36 (1), 4.60 (2)"]
["Koelcapaciteit","Nom.","","","kW","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)"]
["Opgenomen vermogen","Verwarmen","","Nom.","kW","0.830 (1), 1.26 (2)","0.830 (1), 1.26 (2)"]
["","Koelen","","Nom.","kW","0.810 (1), 1.36 (2)","0.810 (1), 1.36 (2)"]
["COP","","","","","5.23 (1), 3.65 (2)","5.23 (1), 3.65 (2)"]
["EER","","","","","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)"]
["Verwarming van sanitair warm water","Algemeen","","Aangegevens belastingprofiel","","L","XL"]
["","Gematigd klimaat","","Energierendementsklasse waterverwarming","","A+","A+"]
["Verwarming","Wateruitlaat gematigd klimaat 55°C","Algemeen","SCOP","","3.29","3.29"]
["","","","Seizoensefficiëntieklasse verwarming","","A++","A++"]
["","Wateruitlaat gematigd klimaat 35°C","Algemeen","SCOP","","4.96","4.96"]
["","","","Seizoensefficiëntieklasse verwarming","","A+++","A+++"]
["Opmerkingen","","","","","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)"]