{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVH-CB / ERHQ-BW17"]
[]
[]
[]
[]
["","","","","EHVH16S18CB3V / ERHQ014BAW17","EHVH16S26CB9W / ERHQ014BAW17"]
["Verwarming van sanitair warm water","Algemeen","Aangegevens belastingprofiel","","L","XL"]
["","Gematigd klimaat","Energierendementsklasse waterverwarming","","A","A"]
["COP","","","","4.24 (1), 3.22 (2)","4.24 (1), 3.22 (2)"]
["Verwarmingscapaciteit","Nom.","","kW","14.5 (1), 13.6 (2)","14.5 (1), 13.6 (2)"]
["Opgenomen vermogen","Verwarmen","Nom.","kW","3.42 (1), 4.21 (2)","3.42 (1), 4.21 (2)"]
["Opmerkingen","","","","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)"]
["","","","","(3) - T. omg. 35°C – Uitgaand water verdamper (LWE) 7°C (DT = 5°C)","(3) - T. omg. 35°C – Uitgaand water verdamper (LWE) 7°C (DT = 5°C)"]
["","","","","(4) - Omgevingstemp. 35°C – Uitgaand water verdamper (LWE) 18℃ (DT = 5°C)","(4) - Omgevingstemp. 35°C – Uitgaand water verdamper (LWE) 18℃ (DT = 5°C)"]
["","","","","(5) - DB/WB 7°C/6°C - Uitgaand water condensor (LWC) 35°C(DT=5°C)","(5) - DB/WB 7°C/6°C - Uitgaand water condensor (LWC) 35°C(DT=5°C)"]
["","","","","(6) - DB/WB 7 °C / 6 °C - Uitgaand water condensor (LWC) 45℃ (Dt=5 °C)","(6) - DB/WB 7 °C / 6 °C - Uitgaand water condensor (LWC) 45℃ (Dt=5 °C)"]