{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBX-AV3"]
[]
[]
[]
[]
["","","","","","EHYHBX08AFV3"]
["Behuizing","Kleur","","","","Wit"]
["","Materiaal","","","","Voorgelakte metaalplaat"]
["Afmetingen","Unit","","Hoogte","mm","902"]
["","","","Breedte","mm","450"]
["","","","Diepte","mm","164"]
["Gewicht","Unit","","","kg","31.2"]
["PED (richtlijn drukapparatuur)","Categorie","","","","Categorie I"]
["Warmtewisselaar waterzijde","Waterdebiet","Verwarmen","Max.","l/min","23.5 (7)"]
["Geluidsvermogenniveau","Nom.","","","dBA","42.0"]
["Werkingsbereik","Verwarmen","waterzijdig","Min.","°C","25 (8)"]
["Werkbereik","Verwarmen","Waterzijde","Max.","°C","55 (8)"]
["","Koelen","Omgeving","Min.","°C DB","10 (8)"]
["","","Waterzijde","Min.","°C","5 (8)"]
["","","","Max.","°C","22 (8)"]
["Voeding","Naam","","","","V3"]
["","Fase","","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50"]
["","Spanning","","","V","230"]
["Draadaansluitingen","Voor aansluiting met gebruikersinterface","","Aantal","","2"]
["","","","Opmerking","","0,75 mm² tot 1,25 mm² (max. lengte 500 m)"]
["Opmerkingen","","","","","(1) - Uitsluitend voor binnenunit"]
["","","","","","(2) - DB/NB 7°C/6°C: uitgaand water condensor 35°C (DT=5°C), boiler overbrugd"]
["","","","","","(3) - DB/NB 7°C/6°C: uitgaand water condensor 45℃ (DT=5°C), boiler overbrugd"]
["","","","","","(4) - Tamb 35°C - LWE 7°C (DT=5°C), boiler overbrugd"]
["","","","","","(5) - Tamb 35°C - LWE 18℃ (DT=5°C), boiler overbrugd"]
["","","","","","(6) - Min. required"]
["","","","","","(7) - Boiler overbrugd"]
["","","","","","(8) - Voor het bedrijfsbereik van *HYHB* en *HYKOMB33AA, zie tekening met bedrijfsbereik"]