{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":7,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYKOMB-AA2"]
[]
[]
[]
[]
["","","","","","EHYKOMB33AA2","EHYKOMB33AA2A"]
["Gas","Aansluiting","","Diameter","mm","15","15"]
["","Verbruik (G20)","","Min","m³/u","0.79","0.79"]
["","","","Max","m³/u","3.39","3.39"]
["","Verbruik (G25)","","Min","m³/u","0.89","0.89"]
["","","","Max","m³/u","3.92","3.92"]
["","Verbruik (G31)","","Min","m³/u","0.30","0.30"]
["","","","Max","m³/u","1.29","1.29"]
["","NOx-klasse","","","","6","6"]
["","NOx-peil (G20)","","","mg/kWu","36","36"]
["Centrale verwarming","Opgenomen warmte Qn (thermische netto-waarde)","Nom","Min","kW","7.6","7.6"]
["","","","Max","kW","27.0","27.0"]
["","Opgenomen warmte Qn (thermische bruto-waarde)","Nom","Min","kW","8.4","8.4"]
["","","","Max","kW","30.0","30.0"]
["","Uitgaand Pn bij 80/60°C","","Min","kW","7.5","7.5"]
["","","","Nom","kW","26.6","26.6"]
["","Centrale verwarming-=-Rendement bij 37/30°C","","Nom","kW","8.2","8.2"]
["","Watertemperatuur","","Max","°C","90","90"]
["Sanitair warm water","Opgenomen warmte (thermische netto-waarde) Qnw","Nom","Min","kW","7.6","7.6"]
["","","","Max","kW","32.7","32.7"]
["","","","Min","kW","8.4","8.4"]
["","","","Max","kW","36.3","36.3"]
["","Comfortklasse (EN13203)","","","","XL","XL"]
["","Temperatuur","","Max","°C","65","65"]
["Toevoerlucht","Concentrisch","","","","nee","nee"]
["Afvoergas","Temperatuur","","Max","°C","70","70"]
["","Aansluiting","","","mm","60","60"]
["","Massadebiet (G20)","","Max","kg/u","54.4","54.4"]
["","Massadebiet (G25)","","Max","kg/u","54.4","54.4"]
["","Massadebiet (G31)","","Max","kg/u","53.6","53.6"]
["Behuizing","Kleur","","","","RAL9010","RAL9010"]
["","Materiaal","","","","Voorgelakte metaalplaat","Voorgelakte metaalplaat"]
["Afmetingen","Unit","Hoogte","Behuizing","mm","710","710"]
["","","","Breedte","mm","450","450"]
["","","","Diepte","mm","240","240"]
["Gewicht","Unit","","Leeg","kg","36","36"]
["Verwarming van sanitair warm water","Algemeen","","Aangegevens belastingprofiel","","XL","XL"]
["","","","Energierendementsklasse waterverwarming","","A","A"]
["Centrale verwarming","Algemeen","","Seizoensrendementsklasse verwarming","","A","A"]