{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":9,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKEQ"]
[]
[]
[]
[]
["","","","","EKEQMCBAV3","EKEQFCBAV3","EKEQMCBV3","EKEQDCBV3","EKEQFCBV3"]
["Buitenunit","","","","VRV","ERQ","VRV","ERQ","ERQ"]
["Toepassing","","","","Multi","Pair","Multi","Pair","Pair"]
["Afmetingen","Unit","Hoogte","mm","132","132","132","132","132"]
["","","Breedte","mm","400","400","400","400","400"]
["","","Diepte","mm","200","200","200","200","200"]
["Gewicht","Unit","","kg","3.6","3.9","3.6","3.6","3.9"]
["Werkingsbereik","Koelen","Min.","°C DB","-10","-10","-10","-10","-10"]
["","","Max.","°C DB","40","40","40","40","40"]
["Standaard-accessoires","Thermistor (R1T)","","","1","0","1","1","0"]
["","Thermistor (R2T/R3T)","","","2","2","2","2","2"]
["","Isolatieplaat","","","2","2","2","2","2"]
["","Rubberhuls","","","2","2","2","2","2"]
["","Draad-draadverbinding","","","6","4","6","6","4"]
["","Montage- en bedieningshandleiding","","","1","1","1","1","1"]
["","Moer","","","9","7","9","8","7"]
["","Kabelbinders","","","6","6","6","6","6"]
["","Capaciteitsinsteladapter","","","8","7","8","7","7"]
["","Sluitplug","","","0","2","0","0","2"]
["Power supply","Naam","","","V3","V3","V3","V3","V3"]
["","Fase","","","1~","1~","1~","1~","1~"]
["","Frequentie","","Hz","50","50","50","50","50"]
["","Spanning","","V","230","230","230","230","230"]