{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":102,"n_cols":7,"rows_kept":102,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHH2E-AV33"]
[]
[]
[]
[]
["","","","","","EKHH2E200AAV33","EKHH2E260AAV33"]
["Sound power level","Sanitair warm water","","Binnenunit","dBA","","53"]
["","","","Outdoor unit","dBA","","52"]
["Sanitair warm water","Algemeen","","Energierendementsklasse waterverwarming","","","A+"]
["","","","Ingest. temp. thermostaat","°C","","55"]
["","","","Aangegevens belastingprofiel","","","XL"]
["","Koud klimaat","","AEC (jaarlijks stroomverbruik)","kWh","","1,826"]
["","Warm klimaat","","AEC (jaarlijks stroomverbruik)","kWh","","1,296"]
["","Gematigd klimaat","","AEC (jaarlijks stroomverbruik)","kWh","","1,323"]
["Equivalent warm water","Max.","","","l","","342"]
["Warmtepomp","Automatic defrost start","","","°C","","-2"]
["","Werkbereik","Omgeving","Min.","°C DB","","-7"]
["","","","Max.","°C DB","","38"]
["","Casing","","Material","","","Deksel: Afwerking bovenkant EPP"]
["","","","Kleur","","","White body / black top"]
["","Systeemdruk","","Max.","bar","","7"]
["","Ontdooimethode","","","","","Actief met warmegasklep"]
["COP","","","","","3.30 (2), 2.88 (1)","3.10 (1), 3.60 (2)"]
["Koelmiddel","GWP","","","","","1,430.0"]
["","Vulling","","","kg","","0.900"]
["","Type","","","","","R-134a"]
["Compressor","Type","","","","","Rotary non-inverter"]
["Afmetingen","Unit","","Diameter","mm","","650"]
["","","","Hoogte","mm","","2,000"]
["Sanitair warm water","Rendement","","Nom","kW","","1.8"]
["Tank","Montage","","Aansluiting op zonne-installatie mogelijk","","","Neen"]
["","Vermogen ingebouwd verwarmingselement","","Nom.","kW","","1.5"]
["","Omkasting","","Materiaal","","","ABS met reliëfdruk"]
["","","","Kleur","","","Wit"]
["","Afmetingen","Unit","Hoogte","mm","","1,500"]
["","Werkbereik","Waterzijde","Max.","°C","","56"]
["","","","Min.","°C","","10"]
["Gewicht","Verpakte unit","","","kg","","115"]
["","Unit","","Leeg","kg","","95"]
["","","","Vol","kg","","349"]
["Montageplaats","","","","","","Binnen"]
["IP class","","","","","","IP-X4"]
["General","Product description","","Lucht/water-warmtepomp","","","Ja"]
["","Gegevens van leverancier/fabrikant","","Naam en adres","","","ELIC - Via Pietro Zorutti 13/14, 33074 Fontanafredda ITALY"]
["Opwarmtijd","Max.","","","uu:mm","","10:14:00, 07:56:46"]
["Warmtepomp","Voeding","","Frequentie","Hz","","50"]
["","","","Maximale bedrijfsstroom","A","","2"]
["","","","Fase","","","1P"]
["","","","Spanning","V","","230"]
["Tank","Voeding","","Fase","","","1P"]
["","","","Frequentie","Hz","","50"]
["","","","Spanning","V","","230"]
["Opmerkingen","","","","","(1) - Conform EN16147-2011, inlaattemperatuur 7°C, kamertemperatuur 20°C, koudwaterinlaat 10°C","(1) - Conform EN16147-2011, inlaattemperatuur 7°C, kamertemperatuur 20°C, koudwaterinlaat 10°C"]
["","","","","","(2) - Conform EN16147-2011, inlaattemperatuur 15°C, kamertemperatuur 20°C, koudwaterinlaat 10°C","(2) - Conform EN16147-2011, inlaattemperatuur 15°C, kamertemperatuur 20°C, koudwaterinlaat 10°C"]
["","","","","","","(3) - Binnentemperatuur: 29°CDB, 19°CWB; buitentemperatuur: 46°CDB, 24°CWB"]
["","","","","","","(4) - Binnentemperatuur: 27°CDB, 19°CWB; buitentemperatuur: 35°CDB, 24°CWB"]
["Opwarmtijd","Max.","","","uu:mm","08:17:00, 06:30:44"]
["Sanitair warm water","Rendement","","Nom","kW","1.8"]
["Equivalent warm water","Max.","","","l","275"]
["Afmetingen","Unit","","Hoogte","mm","1714"]
["","","","Diameter","mm","650"]
["Gewicht","Unit","","Leeg","kg","83"]
["","","","Vol","kg","282"]
["","Verpakte unit","","","kg","103"]
["Montageplaats","","","","","Binnen"]
["IP-klasse","","","","","IP-X4"]
["Compressor","Type","","","","Roterende non-inverter"]
["Koelmiddel","Type","","","","R-134a"]
["","GWP","","","","1430.0"]
["Koudemiddel","Vulling","","","tCO2Eq","1.29"]
["Koelmiddel","Vulling","","","kg","0.900"]
["Warmtepomp","Omkasting","","Kleur","","Witte behuizing/zwarte bovenkant"]
["","Behuizing","","Materiaal","","Deksel: Afwerking bovenkant EPP"]
["","Werkbereik","Omgeving","Min.","°C DB","-7"]
["","","","Max.","°C DB","38"]
["","Ontdooimethode","","","","Actief met warmegasklep"]
["","Automatische start ontdooiing","","","°C","-2"]
["","Systeemdruk","","Max.","bar","7"]
["Tank","Werkbereik","Waterzijde","Max.","°C","56"]
["","","","Min.","°C","10"]
["","Vermogen ingebouwd verwarmingselement ","","Nom.","kW","1.5"]
["","Omkasting","","Kleur","","Wit"]
["","","","Materiaal","","ABS met reliëfdruk"]
["","Afmetingen","Unit","Hoogte","mm","1210"]
["","Montage","","Aansluiting op zonne-installatie mogelijk","","Nee"]
["Algemeen","Productbeschrijving","","Lucht/water-warmtepomp","","Ja"]
["","Gegevens van leverancier/fabrikant","","Naam en adres","","ELIC - Via Pietro Zorutti 13/14, 33074 Fontanafredda ITALY"]
["Verwarming van sanitair warm water","Algemeen","","Aangegevens belastingprofiel","","L"]
["","","","Energierendementsklasse waterverwarming","","A+"]
["Sanitair warm water","Algemeen","","Ingest. temp. thermostaat","°C","55"]
["Geluidsniveau","Sanitair warm water","","Buitenunit","dBA","52"]
["","","","Binnenunit","dBA","53"]
["Verwarming van sanitair warm water","Gematigd klimaat","","AEC (jaarlijks stroomverbruik)","kWh","835"]
["","Koud klimaat","","AEC (jaarlijks stroomverbruik)","kWh","1091"]
["","Warm klimaat","","AEC (jaarlijks stroomverbruik)","kWh","756"]
["Warmtepomp","Voeding","","Fase","","1P"]
["","","","Frequentie","Hz","50"]
["","","","Spanning","V","230"]
["","","","Maximale bedrijfsstroom","A","2"]
["Tank","Voeding","","Fase","","1P"]
["","","","Frequentie","Hz","50"]
["","","","Spanning","V","230"]