{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":71,"n_cols":7,"rows_kept":71,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHHE-CV3"]
[]
[]
[]
[]
["","","","","","EKHHE200CV3","EKHHE260CV3"]
["Sound power level","Sanitair warm water","","Binnenunit","dBA","50","50"]
["","","","Outdoor unit","dBA","49","49"]
["Verwarming van sanitair warm water","Algemeen","","Energierendementsklasse waterverwarming","","A+","A+"]
["","","","Ingest. temp. thermostaat","°C","55","55"]
["","","","Functie voor verwarmen van water tijdens daluren","","Ja","Ja"]
["","","","Aangegevens belastingprofiel","","L","XL"]
["","Koud klimaat","","AEC (jaarlijks stroomverbruik)","kWh","979","1,672"]
["","","","Qelec (dagelijks stroomverbruik)","kWh","2.68","4.58"]
["","Warm klimaat","","Qelec (dagelijks stroomverbruik)","kWh","1.91","3.10"]
["","","","AEC (jaarlijks stroomverbruik)","kWh","698","1,132"]
["","Gematigd klimaat","","Qelec (dagelijks stroomverbruik)","kWh","2.08","3.30"]
["","","","AEC (jaarlijks stroomverbruik)","kWh","758","1,203"]
["Warmtepomp","Werkbereik","Omgeving","Min.","°C DB","-7","-7"]
["","","","Max.","°C DB","43","43"]
["","Casing","","Kleur","","Wit","Wit"]
["","Systeemdruk","","Max.","bar","7","7"]
["","Ontdooimethode","","","","Heet gas-ontdooiing","Heet gas-ontdooiing"]
["","Verwarmingscapaciteit","","","kW","0.43","0.43"]
["","Montage","","Afstand van de muur","mm","200","200"]
["","","","IP-klasse","","IP24","IP24"]
["","Gewicht","","Unit","kg","85","97"]
["","","","Verpakte unit","kg","96","109"]
["","Montageplaats","","","","Enkel binnen","Enkel binnen"]
["","Geluidsdrukniveau","","Fluisterstille nachtstand","dBA","50.0","50.0"]
["","","","Nom.","dBA","50","50"]
["","Naam","","","","EKHHE200CV3","EKHHE260CV3"]
["","Koelmiddel","","GWP","","1,430","1,430"]
["","","","Vulling","kg","1","1"]
["","","","Type","","R-134A","R-134A"]
["","Afmetingen","Unit","Diepte","mm","628","628"]
["","","","Breedte","mm","628","628"]
["","","","Hoogte","mm","1,607","1,892"]
["COP","","","","","4.23","4.23"]
["Koelmiddel","GWP","","","","1,430","1,430"]
["","Vulling","","","kg","1","1"]
["","Type","","","","R-134a","R-134a"]
["Compressor","Type","","","","Roterend","Roterend"]
["Afmetingen","Unit","","Diameter","mm","628","628"]
["","","","Hoogte","mm","1,607","1,892"]
["","","Hoogte","Geïntegreerd in binnenunit","mm","1,607","1,892"]
["Sanitair warm water","Rendement","","Nom","kW","1.82","1.82"]
["Tank","Montage","","Aansluiting op zonne-installatie mogelijk","","Neen","Neen"]
["","","","IP-klasse","","IP24","IP24"]
["","","","Recirculatie-opening tank","","Neen","Neen"]
["","Vermogen ingebouwd verwarmingselement","","Nom.","kW","1.5","1.5"]
["","Montageplaats","","","","Enkel binnen","Enkel binnen"]
["","Omkasting","","Materiaal","","Geëmailleerd staal","Geëmailleerd staal"]
["","","","Kleur","","Wit","Wit"]
["Gewicht","Verpakte unit","","","kg","96","109"]
["","Unit","","Leeg","kg","85","97"]
["Montageplaats","","","","","Binnen","Binnen"]
["Algemeen","LW(A) geluidsvermogensniveau (volgens EN14825)","","Binnen","dB(A)","50","50"]
["","Productbeschrijving","","Lucht/water-warmtepomp","","Ja","Ja"]
["","","","Model identifier","","EKHHE200CV3","EKHHE260CV3"]
["","Gegevens van leverancier/fabrikant","","Naam of handelsmerk","","Daikin Europe N.V.","Daikin Europe N.V."]
["","Extra verwarmingselement","","Type stroomvoorziening","","Elektriciteit","Elektriciteit"]
["Opwarmtijd","Max.","","","uu:mm","08:17:00","10:14:00"]
["Warmtepomp","Voeding","","Frequentie","Hz","50","50"]
["","","","Maximale bedrijfsstroom","A","8.5","8.5"]
["","","","Fase","","1P","1P"]
["","","","Spanning","V","230","230"]
["","","","Aanbevolen plaatselijk gebruik","A","2.43","2.43"]
["Tank","Voeding","","Fase","","1P","1P"]
["","","","Frequentie","Hz","50","50"]
["","","","Spanning","V","230","230"]