{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":10,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHHP-A2V3"]
[]
[]
[]
[]
["","","","","EKHHP300AC2V3","EKHHP500AC2V3","EKHHP300AB2V3 (Archived)","EKHHP500AA2V3 (Archived)","EKHHP300AA2V3 (Archived)","EKHHP500AB2V3 (Archived)"]
["Geluidsdrukniveau","Nom.","","dBA","0","0","0","0","0","0"]
["Koelmiddel","GWP","","","2,087.5","2,087.5","2,087.5","","","2,087.5"]
["","Type","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Sound power level","Nom.","","dBA","39","39","39","0","0","39"]
["Afmetingen","Unit","Breedte","mm","595","790","595","790","615","790"]
["","","Diepte","mm","615","790","615","790","615","790"]
["","","Hoogte","mm","1,772","1,778","1,772","1,750","1,750","1,778"]
["Behuizing","Kleur","","","Verkeerswit (RAL9016)/Donkergrijs (RAL7011)","Verkeerswit (RAL9016)/Donkergrijs (RAL7011)","Verkeerswit (RAL9016)/Donkergrijs (RAL7011)","Verkeerswit (RAL9016)/Donkergrijs (RAL7011)","Verkeerswit (RAL9016)/Donkergrijs (RAL7011)","Verkeerswit (RAL9016)/Donkergrijs (RAL7011)"]
["PED (richtlijn drukapparatuur)","Categorie","","","Categorie I","Categorie I","Categorie I","Categorie I","Categorie I","Categorie I"]
["Gewicht","Unit","","kg","70","80","70","80","70","80"]
["Power supply","Fase","","","1~","1~","1~","3N~","3N~","1~"]
["","Frequentie","","Hz","50","50","50","50","50","50"]
["","Spanning","","V","230","230","230","230","230","230"]
["Stroom","Aanbevolen zekeringen","","A","16","16","16","16","16","16"]
["Opmerkingen","","","","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897","","","(1) - Warmteverlies volgens EN12897"]