{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":6,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWCB-PB"]
[]
[]
[]
[]
["","","","","","EKHWCB500PBA"]
["Montage_","","","","","Vloer"]
["Behuizing","Kleur","","","","Verkeerswit (RAL9016)/Donkergrijs (RAL7011)"]
["","Materiaal","","","","Slagvast polypropyleen"]
["Afmetingen","Unit","Hoogte","Tank","mm","1,660"]
["","","","Breedte","mm","790"]
["","","","Diepte","mm","790"]
["Gewicht","Unit","","Leeg","kg","86"]
["","","","Vol","kg","586"]
["Tank","Watervolume","","","l","477"]
["","Materiaal","","","","Polypropyleen"]
["","Maximumwatertemperatuur","","","°C","85"]
["","Energie-efficiëntieklasse","","","","B"]
["Warmtewisselaar","Sanitair warm water","","Hoeveelheid","","1"]
["","","","Buismateriaal","","Roestvrij staal (DIN 1.4404)"]
["","","","Volume interne spiraal","l","25.8"]
["","","","Bedrijfsdruk","bar","6"]
["","","","Gemiddeld specifiek thermisch vermogen","W/K","2,580"]
["","Vullen","","Hoeveelheid","","1"]
["","","","Buismateriaal","","Roestvrij staal (DIN 1.4404)"]
["","","","Volume interne spiraal","l","9"]
["","","","Bedrijfsdruk","bar","3"]
["","","","Gemiddeld specifiek thermisch vermogen","W/K","1,030"]
["","Hulpzonneverwarming","","Hoeveelheid","","1"]
["","","","Buismateriaal","","Roestvrij staal (DIN 1.4404)"]
["","","","Volume interne spiraal","l","4"]
["","","","Bedrijfsdruk","bar","3"]
["","","","Gemiddeld specifiek thermisch vermogen","W/K","350"]
["Opmerkingen","","","","","(1) - Warmteverlies volgens EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃"]
["","","","","","(5) - Voor een aftapvolume van 140l -> 5820 Wh (bad) / 8kW warmtepomp"]
["","","","","","(6) - Voor een aftapvolume van 90l -> 3660 Wh (bad) / 8kW warmtepomp"]
["","","","","","(7) - Voor een aftapvolume van 140l -> 5820 Wh (bad) / 16kW warmtepomp"]
["","","","","","(8) - Voor een aftapvolume van 90l -> 3660 Wh (bad) / 16kW warmtepomp"]