{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":7,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWET-BV3"]
[]
[]
[]
[]
["","","","","","EKHWET90BAV3","EKHWET120BAV3"]
["Montage_","","","","","Wand","Wand"]
["Behuizing","Kleur","","","","Wilt + zwart","Wilt + zwart"]
["","Materiaal","","","","Metaalplaat, Acrylonitril-butadieen-styreen","Metaalplaat, Acrylonitril-butadieen-styreen"]
["Afmetingen","Unit","Hoogte","Tank","mm","1032","1283"]
["","","","Breedte","mm","510","510"]
["","","","Diepte","mm","570","570"]
["Gewicht","Unit","","Leeg","kg","43","47"]
["Tank","Watervolume","","","l","89","118"]
["","Materiaal","","","","Gemoffeld staal conform DIN4753TL2","Gemoffeld staal conform DIN4753TL2"]
["","Maximumwatertemperatuur","","","°C","75.0","75.0"]
["","Energie-efficiëntieklasse","","","","B","C"]
["Warmtewisselaar","Sanitair warm water","","Hoeveelheid","","1","1"]
["","","","Buismateriaal","","Aluminium","Aluminium"]
["","","","Bedrijfsdruk","bar","42","42"]
["Boosterverwarmer","Capaciteit","","","kW","1.2","1.2"]
["Bereik van het energierendement","","","","","A+ ~ F","A+ ~ F"]