{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EVH"]
[]
[]
[]
[]
["","","","","","ERGA06EAV3H"]
["Afmetingen","Unit","","Hoogte","mm","740"]
["","","","Breedte","mm","884"]
["","","","Diepte","mm","388"]
["Gewicht","Unit","","","kg","58.5"]
["Bedrijfsbereik","Koelen","","Min.","°CDB","10"]
["","","","Max.","°CDB","43"]
["Werkbereik","Sanitair warm water","","Min.","°CDB","-25"]
["","","","Max.","°CDB","35"]
["Geluidsvermogenniveau","Verwarmen","","Nom.","dBA","60 (1)"]
["","Koelen","","Nom.","dBA","62 (1)"]
["Geluidsdrukniveau","Verwarmen","","Nom.","dBA","47 (1)"]
["","Koelen","","Nom.","dBA","49 (1)"]
["Koelmiddel","Type","","","","R-32"]
["","GWP","","","","675.0"]
["Koudemiddel","Vulling","","","tCO2Eq","1.01"]
["Koelmiddel","Vulling","","","kg","1.50"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6"]
["","Gas","","Buitendiameter","mm","15.9"]
["","Afvoer","","UD","mm","18"]
["","Niveauverschil:","IU - OU","Max.","m","30.0"]
["","Thermische isolatie","","","","Zowel vloeistof- als gasleidingen"]
["Voeding","Naam","","","","V3"]
["","Fase","","","","1N~"]
["Spanningsvoeding","Frequentie","","","Hz","50"]
["","Spanning","","","V","230"]
["Stroom","Aanbevolen zekeringen","","","A","20"]
["Opmerkingen","","","","","(1) - Koelen Ta 35°C - LWE 18°C ( DT = 5°C ) - Verwarmen Ta DB/WB 7°C/6°C - LWC 35°C ( DT = 5°C)"]