{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSHB12E"]
[]
[]
[]
[]
["","","","","","ETSHB12P50EG","ETSHB12P30EG","ETSHB12P30EF (Archived)","ETSHB12P50EF (Archived)"]
["Behuizing","Kleur","","","","Wit (RAL9016) / Zwart (RAL9017)","Wit (RAL9016) / Zwart (RAL9017)","Wit (RAL9016) / Zwart (RAL9017)","Wit (RAL9016) / Zwart (RAL9017)"]
["","Materiaal","","","","Slagvast polypropyleen","Slagvast polypropyleen","Slagvast polypropyleen","Slagvast polypropyleen"]
["Afmetingen","Unit","","Hoogte","mm","1910","1891","1892","1910"]
["","","","Breedte","mm","792","594","594","792"]
["","","","Diepte","mm","817","644","644","816"]
["Gewicht","Unit","","","kg","100","76","76","100"]
["Geluidsvermogenniveau","Nom.","","","dBA","47.3","47.3","47.3","47.3"]
["Geluidsdrukniveau","Nom.","","","dBA","38.6","38.6","38.6","38.6"]
["Werkingsbereik","Verwarmen","waterzijdig","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["Werkbereik","Verwarmen","Waterzijde","Max.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","Koelen","Omgeving","Min.","°C DB","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","Waterzijde","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["Voeding","Fase","","","","1~","1~","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50","50","50"]
["","Spanning","","","V","230","230","230","230"]
["Opmerkingen","","","","","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897"]
["","","","","","(2) - Raadpleeg de tekeningen met bedrijfslimieten","(2) - Raadpleeg de tekeningen met bedrijfslimieten","(2) - Raadpleeg de tekeningen met bedrijfslimieten","(2) - Raadpleeg de tekeningen met bedrijfslimieten"]